	USER 1= 
	
	USER 2=
	
	AND
	
	OR

	Single Phase Undervoltage (27-1P)
	
	Three Phase Undervoltage (27-3P)
	
	Single Phase Overvoltage (59)
	
	Three Phase  Overvoltage (59-3P)

	Low Power Factor Alarm (LPFA)
	
	Load Current Alarm (LOADA)
	
	Phase Peak Demand Alarm (PDA)
	
	Neutral Peak Demand Alarm (NDA)

	Directional Power Flow Alarm (32P)
	
	Underfrequency Alarm (81S-1)
	
	Overfrequency Alarm (81O-1)
	
	SWITCH MODE ACTIVE

	Loss of AC Power Alarm (LOAC)
	
	Breaker Failure Alarm (BFA)
	
	Remote Hot Line Tag Applied
	
	Loop Control Trip (LCMTRIP)

	Loop Control Close (LCMCLOSE)
	
	PROG 1: Battery Test

PROG 2: N/A (future). 
	
	This Recloser is Set to 

1( Trip,  3(. Lockout.
	
	This Recloser is Set to 

1( Trip,  1(. Lockout.

	LABELS for PCD USER LED’s, PROG Buttons, and Trip Mode ID.  See PCD Inst. Book for setting information.
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