Item	Qty.	Description	Price per	Amount
			unit

	Manual Call Point, blue, changeover contact	Carry:

	The Manual Call Point HM/A 2.1 is designed for connection to a conventional DC threshold alarm
	detector zone. The Manual Call Point latches.
	A visual display indicates the Manual Call Point’s state.
	The Manual Call Point possesses an additional changeover switch.
	The Manual Call Point can be used as a button simply by removing the locking lever.
	Both SM and FM cable entries are available for the cabling.

	Operating voltage	10 – 30 V DC
				(supplied by the zone)
	Contact load of switch S2	< 25 V AC / 2 A or
				< 60 V DC / 2 A
	Dimensions (W x H x D)	126 x 126 x 35 mm
	Connection	Screw terminals
				Max. 1.5 mm²
	Cable entry point
		Top and bottom	2 pcs. M20 x 1.5 mm
		Rear wall	2 pcs. 24 x 10 mm
	Weight	420 g
	Degree of protection	IP43
	Rel. humidity	5 – 95%
				(non-condensing)
	Ambient temperature	-20 to +60 °C
				(continuous operation, without icing)
				-25 to +70 °C (max. 12 hours)

	Manufacturer:	ABB STOTZ-KONTAKT

	Type:	HM/A 2.1

	Material:..........	Labor:..........

				HMA_21_AT_EN_V2-0
				9AKK107991A0090 Rev. A	Carry: