{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["BOM","Data"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":78,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"BOM","index":0,"n_rows":18,"n_cols":3,"rows_kept":18,"cut":false,"hidden":false,"merged":[]}
["Quantity","Part Number","Description"]
[null,null,"Please verify BOM for Accuracy.  Optional items have been added for your convenience, if these optional items are not needed, please remove them from the BOM before placing your order!"]
[null,null,"Magne"]
[2,"2TLA042022R3000","Magne 4X DYN M12-5 connector"]
[null,null,"Eva"]
[2,"2TLA020046R0900","Eva Unique Code, One of 1,000 codes, complies with EN/ISO 14119"]
[null,null,"Anchor Plate"]
[2,"2TLA042023R0400","Magne Anchor plate 32B with magnet"]
[null,null,"Magne door Hardware"]
[2,"2TLA042023R0500","JSM D21B - Mounting Kit for Magne on Conventional Door"]
[2,"2TLA042023R0100","JSM D28 - Handle Profile for Magne on Conventional Door"]
[2,"2TLA042023R0300","JSM D24 - Mounting Kit for Eva on Conventional Door"]
[2,"2TLA042023R1000","JSM D27 Handle and screws for JSM D21"]
[null,null,"Cable(s) for your Magne"]
[2,"2TLA020056R0000","M12-C61 5 Pin Female M-12 Cable 6 Meters"]
[2,"2TLA020056R1000","M12-C101 5 Pin Female M-12 Cable 10 Meters"]
[2,"2TLA020056R1400","M12-C201 5 Pin Female M-12 Cable 20 Meters"]
[null,null,"*Note, you do not need 1 of each cable length. Please select the appropriate cable length for your application"]

{"sheet":"Data","index":1,"n_rows":163,"n_cols":2,"rows_kept":163,"cut":false,"hidden":false,"merged":[[151,0,151,1],[159,0,159,1],[120,0,120,1],[125,0,125,1],[109,0,109,1],[145,0,145,1],[116,0,116,1],[141,0,141,1],[132,0,132,1],[137,0,137,1],[104,0,104,1],[1,0,1,1],[8,0,8,1],[95,0,95,1],[87,0,87,1],[77,0,77,1],[25,0,25,1],[33,0,33,1],[45,0,45,1],[62,0,62,1],[18,0,18,1]]}
[]
["5 Pin Female Cables"]
["Part Number","Description"]
["ALL","ALL"]
["2TLA020056R0000","M12-C61 5 Pin Female M-12 Cable 6 Meters"]
["2TLA020056R1000","M12-C101 5 Pin Female M-12 Cable 10 Meters"]
["2TLA020056R1400","M12-C201 5 Pin Female M-12 Cable 20 Meters"]
[]
["5 Pin  M/F Cables"]
["Part Number","Description"]
["ALL","ALL"]
["2TLA020056R5800","M12-C0312 5 Pin Male/Female M-12 Cable 0.3 Meters"]
["2TLA020056R2000","M12-C112 5 Pin Male/Female M-12 Cable 1 Meter"]
["2TLA020056R2100","M12-C312 5 Pin Male/Female M-12 Cable 3 Meters"]
["2TLA020056R2200","M12-C612 5 Pin Male/Female M-12 Cable 6 Meters"]
["2TLA020056R2300","M12-C1012 5 Pin Male/Female M-12 Cable 10 Meters"]
["2TLA020056R2400","M12-C2012 5 Pin Male/Female M-12 Cable 20 Meters"]
[]
["8 Pin Female Cables"]
["Part Number","Description"]
["ALL","ALL"]
["2TLA020056R3000","M12-C63 8 Pin Female M-12 Cable 6 Meters"]
["2TLA020056R4000","M12-C103 8 Pin Female M-12 Cable 10 Meters"]
["2TLA020056R4100","M12-C203 8 Pin Female M-12 Cable 20 Meters"]
[]
["Sentry Safety Relays"]
["Part Number","Description"]
["2TLA010050R0000","SSR10 3NO+1NC Safety Outputs, 24VDC Coil, Manual or Auto Reset"]
["2TLA010052R0400","SSR32 2NO+2NO Delayed Safety Outputs (0.5s), 24VDC Coil, Manual or Auto Reset"]
["2TLA010053R0400","SSR42 2NO+2NO Delayed Safety Outputs (1.5s), 24VDC Coil, Manual or Auto Reset"]
["2TLA010070R0000","USR10 3NO+1NC Configurable Safety Outputs, 24VDC Coil, Manual or Auto Reset"]
["2TLA010070R0400","USR22 Universal Safety Relay 4NO Safety Outputs, 24VDC Coil, Manual or Auto Reset"]
[]
["Pluto Safety PLC"]
["Part Number","Description"]
["2TLA020070R4700","Pluto S20, Safety PLC with 8 failsafe inputs plus 8 non-failsafe outputs/failsafe inputs plus 2 individual failsafe relay outputs plus 2 individually failsafe transistor outputs."]
["2TLA020070R1800","Pluto S46, Safety PLC with 24 failsafe inputs plus 16 non-failsafe outputs or failsafe inputs plus 4 individual failsafe relay outputs plus 2 individually failsafe transistor outputs"]
["2TLA020070R4600","Pluto B20, Safety PLC with 8 failsafe inputs plus 8 non-failsafe outputs/failsafe inputs plus 2 individual failsafe relay outputs plus 2 individually failsafe transistor outputs. For use with Pluto safe bus and/or a Pluto Safety databus."]
["2TLA020070R4800","Pluto B22, Safety PLC with 14 failsafe inputs plus 8 non-failsafe outputs/failsafe inputs. For use with Pluto safe bus and/or a Pluto Safety databus."]
["2TLA020070R1700","Pluto B46, Safety PLC with 24 failsafe inputs plus 16 non-failsafe outputs/failsafe inputs plus 4 individual failsafe relay outputs plus 2 individually failsafe transistor outputs"]
["2TLA020070R6400","Pluto D20, Safety PLC with 8 failsafe inputs plus 8 non-failsafe outputs/failsafe inputs plus 2 individual failsafe relay outputs plus 2 individually failsafe transistor outputs. For use with Pluto safe bus and/or a Pluto Safety databus. 4 analog in."]
["2TLA020070R6600","Pluto D45, Safety PLC with 24 failsafe in plus 15 non-failsafe out/failsafe in plus 4 individual failsafe relay out plus 2 individually failsafe transistor out. 8 analog inputs, 4 high speed counter in."]
["2TLA020070R1100","Pluto AS-I V2 Safety PLC with 4 failsafe inputs and 4 non-failsafe outputs or failsafe inputs and 2 individual failsafe relay outputs and 2 individual failsafe transistor outputs "]
["2TLA020070R1400","Pluto B42 AS-I, Safety PLC with 20 failsafe inputs and 16 non-failsafe outputs or failsafe inputs and 4 individual failsafe relay outputs and 2 individual failsafe transistor outputs "]
[]
["Pluto Safety PLC Accesssories - All Versions Except S"]
["Part Number","Description"]
["2TLA020071R9000","GATE-EIP, Gateway for 2-way communication between the Pluto bus and Ethernet/IP"]
["2TLA020071R9300","GATE-PN, Gateway for 2-way communication between the Pluto bus and ProfiNet"]
["2TLA020071R9400","GATE-MT, Gateway for 2-way communication between the Pluto bus and Modbus TCP"]
["2TLA020071R9200","GATE-S3, Gateway for 2-way communication between the Pluto bus and Sercos III"]
["2TLA020071R9100","GATE-EC, Gateway for 2-way communication between the Pluto bus and EtherCat"]
["2TLA020070R8500","Pluto O2, Output module with Pluto safety bus. Safety output module. Totally 6 I/O: 2 Failsafe inputs for monitoring + 2 non-failsafe outputs/failsafe inputs + 2 individually failsafe relay outputs (with 3 contacts each)"]
["2TLA020070R2000","IDFIX-R, Identifier, read only. For assigning Pluto an address on the Pluto bus"]
["2TLA020070R2100 ","IDFIX-RW, Identifier, read/write. For assigning Pluto an address on the Pluto bus"]
["2TLA020070R2400","IDFIX-PROG 2k5, External memory, 2.5 kbyte. For projects with only one Pluto, store the PLC program, required for Pluto Bus"]
["2TLA020070R2600","IDFIX-PROG 10k, External memory, 10 kbyte. For projects with only one Pluto, store the PLC program, required for Pluto Bus "]
["2TLA020070R2200","R-120, Terminating resistor for Pluto bus."]
["2TLA020070R6805","CAN-Bus cable, 50M, yellow, 1 x 2 x 0.75 mm, 100/500M see cable section"]
["2TLA020070R5700","Programming Cable HMI, Cable for connecting HMI-panel to Pluto programming port"]
["2TLA020070R5800","Programming Cable USB, For connecting PC, USB port to Pluto for programming with Pluto Manager"]
[]
["Safety Contactors"]
["Part Number","Description"]
[null,"None"]
["AFS09Z-30-22-30","AFS09Z-30-22-30 Safety Contactor, 24VDC Coil, 5HP, 25AMP AC-1, 4KW AC-3"]
["AFS12Z-30-22-30","AFS12Z-30-22-30 Safety Contactor, 24VDC Coil, 7.5HP, 28AMP AC-1, 5.5KW AC-3"]
["AFS16Z-30-22-30","AFS16Z-30-22-30 Safety Contactor, 24VDC Coil, 10HP, 30AMP AC-1, 7.5KW AC-3"]
["AFS26Z-30-22-30","AFS26Z-30-22-30 Safety Contactor, 24VDC Coil, 15HP, 45AMP AC-1, 11KW AC-3"]
["AFS30Z-30-22-30","AFS30Z-30-22-30 Safety Contactor, 24VDC Coil, 20HP, 50AMP AC-1, 15KW AC-3"]
["AFS38Z-30-22-30","AFS38Z-30-22-30 Safety Contactor, 24VDC Coil, 25HP, 50AMP AC-1, 18.5KW AC-3"]
["AFS40-30-22-11","AFS40-30-22-11 Safety Contactor, 20-60VDC Coil, 30HP, 70AMP AC-1, 18.5KW AC-3"]
["AFS52-30-22-11","AFS52-30-22-11 Safety Contactor, 20-60VDC Coil, 40HP, 100AMP AC-1, 22KW AC-3"]
["AFS65-30-22-11","AFS65-30-22-11 Safety Contactor, 20-60VDC Coil, 50HP, 105AMP AC-1, 30KW AC-3"]
["AFS80-30-22-11","AFS80-30-22-11 Safety Contactor, 20-60VDC Coil, 60HP, 125AMP AC-1, 37KW AC-3"]
["AFS96-30-22-11","AFS96-30-22-11 Safety Contactor, 20-60VDC Coil, 60HP, 130AMP AC-1, 45KW AC-3"]
[]
["Expansion Relays"]
["Part Number","Description"]
[null,"None"]
["2TLA010040R0000","BSR10 3NO+1NC Safety Contacts, 24VDC Coil"]
["2TLA010040R0200","BSR11 4NO Safety Contacts, 24VDC Coil"]
["2TLA010041R0600","BSR23 4NO+1NC Safety Contacts, 24VDC Coil"]
["2TLA010060R0000","TSR10 3NO+1NC Safety Contacts, 0-999S Off Delay, 24VDC Coil"]
["2TLA010061R0000","TSR20 3NO+1NC Safety Contacts, 0.5s & 1.5S Off Delay, 24VDC Coil"]
[]
[]
["Reset Buttons"]
["Part Number","Description"]
["2TLA030053R0000","Smile 11 RA Reset button 1xNO with M12 male"]
["2TLA030053R0100","Smile 11 RB Pluto Reset button 1xNO with M12 male"]
[]
[]
[]
[]
["Pluto Safety PLC Accesssories - S Versions Only"]
["Part Number","Description"]
["2TLA020070R2000","IDFIX-R, Identifier, read only. For assigning Pluto an address on the Pluto bus"]
["2TLA020070R2100 ","IDFIX-RW, Identifier, read/write. For assigning Pluto an address on the Pluto bus"]
["2TLA020070R2400","IDFIX-PROG 2k5, External memory, 2.5 kbyte. For projects with only one Pluto, store the PLC program, required for Pluto Bus"]
["2TLA020070R2600","IDFIX-PROG 10k, External memory, 10 kbyte. For projects with only one Pluto, store the PLC program, required for Pluto Bus "]
["2TLA020070R5700","Programming Cable HMI, Cable for connecting HMI-panel to Pluto programming port"]
["2TLA020070R5800","Programming Cable USB, For connecting PC, USB port to Pluto for programming with Pluto Manager"]
[]
["Vital"]
["Part Number","Description"]
["2TLA020052R1000","Vital 1 Controller, 2 NO Safety Outputs, 24VDC Coil"]
[]
[]
["8 Pin M/F Cables"]
["Part Number","Description"]
["ALL","ALL"]
["2TLA020056R6400","M12-C00612 8 Pin Male/Female M-12 Cable 60 MM"]
["2TLA020056R5000","M12-C134 8 Pin Male/Female M-12 Cable 1 Meter"]
["2TLA020056R5100","M12-C334 8 Pin Male/Female M-12 Cable 3 Meters"]
[]
["Local Reset Buttons"]
["Part Number","Description"]
["2TLA030053R2700","Smile 12RG - Reset button in Smile enclosure for local reset of Adam Reset M12-8. Blue LED, M12-8 male + female connectors."]
[]
["M12 Adapters"]
["Part Number","Description"]
["2TLA020055R0600","M12-3S, Y-Connector 5 Pin, (1) 5 Pin to Magne, (2) 5 Pin for series connection"]
["2TLA020055R0700","M12-3G, Y-Connector 8 Pin, (1) 8 Pin to Magne, (2) 8 Pin for series connection"]
[]
["Magne 4"]
["Part Number","Description"]
["2TLA042022R3000","Magne 4X DYN M12-5 connector"]
["2TLA042022R3400","Magne 4 DYN-Info M12-8 connector"]
["2TLA042022R3410","Magne 4 DYN-2Info M12-8 connector"]
["2TLA042022R4600","Magne 4 OSSD-Info M12-8 connector"]
[]
["Eva"]
["Part Number","Description"]
["2TLA020046R0800","Eva General Code, All Generals have the same code"]
["2TLA020046R0900","Eva Unique Code, One of 1,000 codes, complies with EN/ISO 14119"]
[]
["Mounting Bracket"]
["Part Number","Description"]
["2TLA040033R3600","JSMD4H Eden mounting plate (2 req, 1 per Adam/Eva)"]
[]
["Terminator"]
["Part Number","Description"]
["2TLA020053R7100","JSOP-2  8 Pin Terminator for M12-3G serial connector"]
[]
["5 Pin Male Cables"]
["Part Number","Description"]
["ALL","ALL"]
["2TLA020056R0200","M12-C62 5 Pin Male M-12 Cable 6 Meters"]
["2TLA020056R1200","M12-C102 5 Pin Male M-12 Cable 10 Meters"]
[]
["Magne Mounting Brackets"]
["Part Number","Description"]
["2TLA042023R0200","JSM D23 - Mounting Kit for Magne on Sliding Door"]
["2TLA042023R0500","JSM D21B - Mounting Kit for Magne on Conventional Door"]
["2TLA042023R0100","JSM D28 - Handle Profile for Magne on Conventional Door"]
["2TLA042023R0300","JSM D24 - Mounting Kit for Eva on Conventional Door"]
["2TLA042023R1000","JSM D27 Handle and screws for JSM D21"]
[]
["Magne Anchor Plates"]
["Part Number","Description"]
["2TLA042023R1300","Magne Anchor plate 32A without magnet"]
["2TLA042023R0400","Magne Anchor plate 32B with magnet"]