;Width Safe##LENGTH##MILLIMETERS;Width (mm)##LENGTH##MILLIMETERS;Wholesaler Art. No.##OTHER##;Wholesaler##OTHER##;White##OTHER##;Watermarked By##OTHER##;Wall Thickness##LENGTH##MILLIMETERS;Wall Mounted##OTHER##;Upper Width 4##LENGTH##MILLIMETERS;Upper Width 3##LENGTH##MILLIMETERS;Upper Width 2##LENGTH##MILLIMETERS;Upper Width 1##LENGTH##MILLIMETERS;URL##OTHER##;Trim Frame Visible##OTHER##;Top Clearance##LENGTH##MILLIMETERS;Stabu Code##OTHER##;Space Units [SU]##OTHER##;Show Service Space Safe##OTHER##;Show Service Area Inside Wall##OTHER##;Show Service Area##OTHER##;Right Clearance##LENGTH##MILLIMETERS;Revit Version##OTHER##;Rated Current In [A]##OTHER##;RAL-Number##OTHER##;Protection Class##OTHER##;Product Line##OTHER##;Phase##OTHER##;Panel Width (PW)##OTHER##;Grid Units (GU)##OTHER##;Material of Enclosures##OTHER##;Manufacturer URL##OTHER##;Manufacturer Art. No.##OTHER##;MEPcontent Class##OTHER##;Left Clearance##LENGTH##MILLIMETERS;Internal Art. No.##OTHER##;IFCExportType##OTHER##;IFCExportAs##OTHER##;Hole Width##LENGTH##MILLIMETERS;Hole Height##LENGTH##MILLIMETERS;Hole Depth##LENGTH##MILLIMETERS;Height (mm)##LENGTH##MILLIMETERS;Handle Height##LENGTH##MILLIMETERS;Handle##OTHER##;Half Width##LENGTH##MILLIMETERS;GTIN##OTHER##;GLN##OTHER##;Function Code##OTHER##;Front Clearance##LENGTH##MILLIMETERS;Flush Mounted##OTHER##;Family Version##OTHER##;Interior Fitting##OTHER##;ETIM Article Class##OTHER##;EMCS Version##OTHER##;Double Door##OTHER##;Model##OTHER##;Manufacturer##OTHER##;Door Width 2##LENGTH##MILLIMETERS;Door Type##OTHER##;Door Opening Angle [degrees]##OTHER##;Description##OTHER##;Depth (mm)##LENGTH##MILLIMETERS;Degree of Protection##OTHER##;Custom##OTHER##;Copyright##OTHER##;Content Supplier URL##OTHER##;Connection Voltage##ELECTRICAL_POTENTIAL##VOLTS;CB-NL Class##OTHER##;Bottom Width##LENGTH##MILLIMETERS;Bottom Clearance##LENGTH##MILLIMETERS;Base Family Version##OTHER##;Back Clearance##LENGTH##MILLIMETERS;Article Type##OTHER##;Article Description##OTHER##;Area of Application##OTHER##;Trim Frame Type##OTHER##;Class of Protection with Accessories##OTHER##;Rated Operational Voltage Ue [V] AC##OTHER##;Locking Type — Lock##OTHER##
A17 - IP44 84 modules 1100x300x215;276.8;300;;;Color RAL 9016;www.stabiplan.com;12.5;1;111.3;111.3;111.3;111.3;www.stabiplan.com;0;300;;84;0;0;0;300;2017;250;9016;Double insulated;ABB;3;1;7;Sheet steel;https://new.abb.com/products/2CPX052030R9999;2CPX052030R9999;DISTRIBUTION_PANEL;250;;IfcElectricDistributionPoint;DISTRIBUTIONBOARD;275;1075;202.5;1100;467.5;1;137.5;;;E6211;300;0;12.11;Pre-assembled for installation of metering-, modules, Combi-Sets, CombiLine-Module on EDF-mounting frame;EC000248;4;0;A17 - IP44 84 modules 1100x300x215;ABB;275;Metal door;120;A17 Wall Cabinet 1PW7R PC2 IP44;215;IP44;0;© Stabiplan International BV;www.MEPcontent.com;400;;249.8;500;12.11;60;A17 - IP44 84 modules 1100x300x215;A17 Wall Cabinet 1PW7R PC2 IP44;Internal use;E_Distribution Panel_MEPcontent_ABB_Trim Frame CR17-57_INT-EN_Shared : CR17;;;
A27 - IP44 168 modules 1100x550x215;526.8;550;;;Color RAL 9016;www.stabiplan.com;12.5;1;111.3;111.3;111.3;361.3;www.stabiplan.com;0;300;;168;0;0;0;550;2017;250;9016;Double insulated;ABB;3;2;7;Sheet steel;https://new.abb.com/products/2CPX052031R9999;2CPX052031R9999;DISTRIBUTION_PANEL;250;;IfcElectricDistributionPoint;DISTRIBUTIONBOARD;275;1075;202.5;1100;467.5;1;137.5;;;E6211;550;0;12.11;Pre-assembled for installation of metering-, modules, Combi-Sets, CombiLine-Module on EDF-mounting frame;EC000248;4;0;A27 - IP44 168 modules 1100x550x215;ABB;525;Metal door;120;A27 Wall Cabinet 2PW7R PC2 IP44;215;IP44;0;© Stabiplan International BV;www.MEPcontent.com;400;;249.8;500;12.11;60;A27 - IP44 168 modules 1100x550x215;A27 Wall Cabinet 2PW7R PC2 IP44;Internal use;E_Distribution Panel_MEPcontent_ABB_Trim Frame CR17-57_INT-EN_Shared : CR27;;;
A37 - IP44 252 modules 1100x800x215;776.8;800;;;Color RAL 9016;www.stabiplan.com;12.5;1;111.3;111.3;611.3;361.3;www.stabiplan.com;0;300;;252;0;0;0;550;2017;250;9016;Double insulated;ABB;3;3;7;Sheet steel;https://new.abb.com/products/2CPX052032R9999;2CPX052032R9999;DISTRIBUTION_PANEL;300;;IfcElectricDistributionPoint;DISTRIBUTIONBOARD;275;1075;202.5;1100;467.5;1;137.5;;;E6211;550;0;12.11;Pre-assembled for installation of metering-, modules, Combi-Sets, CombiLine-Module on EDF-mounting frame;EC000248;4;1;A37 - IP44 252 modules 1100x800x215;ABB;249.1;Metal door;120;A37 Wall Cabinet 3PW7R PC2 IP44;215;IP44;0;© Stabiplan International BV;www.MEPcontent.com;400;;249.8;500;12.11;60;A37 - IP44 252 modules 1100x800x215;A37 Wall Cabinet 3PW7R PC2 IP44;Internal use;E_Distribution Panel_MEPcontent_ABB_Trim Frame CR17-57_INT-EN_Shared : CR37;;;
A47 - IP44 336 modules 1100x1050x215;1026.8;1050;;;Color RAL 9016;www.stabiplan.com;12.5;1;111.3;861.3;611.3;361.3;www.stabiplan.com;0;300;;336;0;0;0;550;2017;250;9016;Double insulated;ABB;3;4;7;Sheet steel;https://new.abb.com/products/2CPX052033R9999;2CPX052033R9999;DISTRIBUTION_PANEL;550;;IfcElectricDistributionPoint;DISTRIBUTIONBOARD;275;1075;202.5;1100;467.5;1;137.5;;;E6211;550;0;12.11;Pre-assembled for installation of metering-, modules, Combi-Sets, CombiLine-Module on EDF-mounting frame;EC000248;4;1;A47 - IP44 336 modules 1100x1050x215;ABB;499.1;Metal door;120;A47 Wall Cabinet 4PW7R PC2 IP44;215;IP44;0;© Stabiplan International BV;www.MEPcontent.com;400;;249.8;500;12.11;60;A47 - IP44 336 modules 1100x1050x215;A47 Wall Cabinet 4PW7R PC2 IP44;Internal use;E_Distribution Panel_MEPcontent_ABB_Trim Frame CR17-57_INT-EN_Shared : CR47;;;
A57 - IP44 420 modules 1100x1300x215;1276.8;1300;;;Color RAL 9016;www.stabiplan.com;12.5;1;1111.3;861.3;611.3;361.3;www.stabiplan.com;0;300;;420;0;0;0;800;2017;250;9016;Double insulated;ABB;3;5;7;Sheet steel;https://new.abb.com/products/2CPX052034R9999;2CPX052034R9999;DISTRIBUTION_PANEL;550;;IfcElectricDistributionPoint;DISTRIBUTIONBOARD;275;1075;202.5;1100;467.5;1;137.5;;;E6211;800;0;12.11;Pre-assembled for installation of metering-, modules, Combi-Sets, CombiLine-Module on EDF-mounting frame;EC000248;4;1;A57 - IP44 420 modules 1100x1300x215;ABB;499.1;Metal door;120;A57 Wall Cabinet 5PW7R PC2 IP44;215;IP44;0;© Stabiplan International BV;www.MEPcontent.com;400;;249.8;500;12.11;60;A57 - IP44 420 modules 1100x1300x215;A57 Wall Cabinet 5PW7R PC2 IP44;Internal use;E_Distribution Panel_MEPcontent_ABB_Trim Frame CR17-57_INT-EN_Shared : CR57;;;
A17D - IP54 84 modules 1100x300x215;276.8;300;;;Color RAL 9016;www.stabiplan.com;12.5;1;111.3;111.3;111.3;111.3;www.stabiplan.com;0;300;;84;0;0;0;300;2017;250;9016;Double insulated;ABB;3;1;7;Sheet steel;https://new.abb.com/products/2CPX052100R9999;2CPX052100R9999;DISTRIBUTION_PANEL;250;;IfcElectricDistributionPoint;DISTRIBUTIONBOARD;275;1075;202.5;1100;467.5;1;137.5;;;E6211;300;0;12.11;Pre-assembled for installation of metering-, modules, Combi-Sets, CombiLine-Module on EDF-mounting frame;EC000058;4;0;A17D - IP54 84 modules 1100x300x215;ABB;275;Metal door;120;A17D Wall Cabinet 1PW7R PC2 IP54;215;IP54;0;© Stabiplan International BV;www.MEPcontent.com;400;;249.8;500;12.11;60;A17D - IP54 84 modules 1100x300x215;A17D Wall Cabinet 1PW7R PC2 IP54;Internal use;E_Distribution Panel_MEPcontent_ABB_Trim Frame CR17-57_INT-EN_Shared : CR17;;;
A27D - IP54 168 modules 1100x550x215;526.8;550;;;Color RAL 9016;www.stabiplan.com;12.5;1;111.3;111.3;111.3;361.3;www.stabiplan.com;0;300;;168;0;0;0;550;2017;250;9016;Double insulated;ABB;3;2;7;Sheet steel;https://new.abb.com/products/2CPX052101R9999;2CPX052101R9999;DISTRIBUTION_PANEL;250;;IfcElectricDistributionPoint;DISTRIBUTIONBOARD;275;1075;202.5;1100;467.5;1;137.5;;;E6211;550;0;12.11;Pre-assembled for installation of metering-, modules, Combi-Sets, CombiLine-Module on EDF-mounting frame;EC000058;4;0;A27D - IP54 168 modules 1100x550x215;ABB;525;Metal door;120;A27D Wall Cabinet 2PW7R PC2 IP54;215;IP54;0;© Stabiplan International BV;www.MEPcontent.com;400;;249.8;500;12.11;60;A27D - IP54 168 modules 1100x550x215;A27D Wall Cabinet 2PW7R PC2 IP54;Internal use;E_Distribution Panel_MEPcontent_ABB_Trim Frame CR17-57_INT-EN_Shared : CR27;;;
A37D - IP54 252 modules 1100x800x215;776.8;800;;;Color RAL 9016;www.stabiplan.com;12.5;1;111.3;111.3;611.3;361.3;www.stabiplan.com;0;300;;252;0;0;0;550;2017;250;9016;Double insulated;ABB;3;3;7;Sheet steel;https://new.abb.com/products/2CPX052102R9999;2CPX052102R9999;DISTRIBUTION_PANEL;300;;IfcElectricDistributionPoint;DISTRIBUTIONBOARD;275;1075;202.5;1100;467.5;1;137.5;;;E6211;550;0;12.11;Pre-assembled for installation of metering-, modules, Combi-Sets, CombiLine-Module on EDF-mounting frame;EC000058;4;1;A37D - IP54 252 modules 1100x800x215;ABB;249.1;Metal door;120;A37D Wall Cabinet 3PW7R PC2 IP54;215;IP54;0;© Stabiplan International BV;www.MEPcontent.com;400;;249.8;500;12.11;60;A37D - IP54 252 modules 1100x800x215;A37D Wall Cabinet 3PW7R PC2 IP54;Internal use;E_Distribution Panel_MEPcontent_ABB_Trim Frame CR17-57_INT-EN_Shared : CR37;;;
A47D - IP54 336 modules 1100x1050x215;1026.8;1050;;;Color RAL 9016;www.stabiplan.com;12.5;1;111.3;861.3;611.3;361.3;www.stabiplan.com;0;300;;336;0;0;0;550;2017;250;9016;Double insulated;ABB;3;4;7;Sheet steel;https://new.abb.com/products/2CPX052103R9999;2CPX052103R9999;DISTRIBUTION_PANEL;550;;IfcElectricDistributionPoint;DISTRIBUTIONBOARD;275;1075;202.5;1100;467.5;1;137.5;;;E6211;550;0;12.11;Pre-assembled for installation of metering-, modules, Combi-Sets, CombiLine-Module on EDF-mounting frame;EC000058;4;1;A47D - IP54 336 modules 1100x1050x215;ABB;499.1;Metal door;120;A47D Wall Cabinet 4PW7R PC2 IP54;215;IP54;0;© Stabiplan International BV;www.MEPcontent.com;400;;249.8;500;12.11;60;A47D - IP54 336 modules 1100x1050x215;A47D Wall Cabinet 4PW7R PC2 IP54;Internal use;E_Distribution Panel_MEPcontent_ABB_Trim Frame CR17-57_INT-EN_Shared : CR47;;;
A57D - IP54 420 modules 1100x1300x215;1276.8;1300;;;Color RAL 9016;www.stabiplan.com;12.5;1;1111.3;861.3;611.3;361.3;www.stabiplan.com;0;300;;420;0;0;0;800;2017;250;9016;Double insulated;ABB;3;5;7;Sheet steel;https://new.abb.com/products/2CPX052104R9999;2CPX052104R9999;DISTRIBUTION_PANEL;550;;IfcElectricDistributionPoint;DISTRIBUTIONBOARD;275;1075;202.5;1100;467.5;1;137.5;;;E6211;800;0;12.11;Pre-assembled for installation of metering-, modules, Combi-Sets, CombiLine-Module on EDF-mounting frame;EC000058;4;1;A57D - IP54 420 modules 1100x1300x215;ABB;499.1;Metal door;120;A57D Wall Cabinet 5PW7R PC2 IP54;215;IP54;0;© Stabiplan International BV;www.MEPcontent.com;400;;249.8;500;12.11;60;A57D - IP54 420 modules 1100x1300x215;A57D Wall Cabinet 5PW7R PC2 IP54;Internal use;E_Distribution Panel_MEPcontent_ABB_Trim Frame CR17-57_INT-EN_Shared : CR57;;;
