;Width Safe##LENGTH##MILLIMETERS;Width (mm)##LENGTH##MILLIMETERS;Wholesaler Art. No.##OTHER##;Wholesaler##OTHER##;White##OTHER##;Watermarked By##OTHER##;Wall Thickness##LENGTH##MILLIMETERS;Wall Mounted##OTHER##;Upper Width 4##LENGTH##MILLIMETERS;Upper Width 3##LENGTH##MILLIMETERS;Upper Width 2##LENGTH##MILLIMETERS;Upper Width 1##LENGTH##MILLIMETERS;URL##OTHER##;Trim Frame Visible##OTHER##;Top Clearance##LENGTH##MILLIMETERS;Stabu Code##OTHER##;Space Units [SU]##OTHER##;Show Service Space Safe##OTHER##;Show Service Area Inside Wall##OTHER##;Show Service Area##OTHER##;Right Clearance##LENGTH##MILLIMETERS;Revit Version##OTHER##;Rated Current In [A]##OTHER##;RAL-Number##OTHER##;Protection Class##OTHER##;Product Line##OTHER##;Phase##OTHER##;Number of Rows##OTHER##;Panel Width (PW)##OTHER##;Grid Units (GU)##OTHER##;Material of Enclosures##OTHER##;Manufacturer URL##OTHER##;Manufacturer Art. No.##OTHER##;MEPcontent Class##OTHER##;Left Clearance##LENGTH##MILLIMETERS;Internal Art. No.##OTHER##;IFCExportType##OTHER##;IFCExportAs##OTHER##;Hole Width##LENGTH##MILLIMETERS;Hole Height##LENGTH##MILLIMETERS;Hole Depth##LENGTH##MILLIMETERS;Height (mm)##LENGTH##MILLIMETERS;Handle Height##LENGTH##MILLIMETERS;Handle##OTHER##;Half Width##LENGTH##MILLIMETERS;GTIN##OTHER##;GLN##OTHER##;Function Code##OTHER##;Front Clearance##LENGTH##MILLIMETERS;Flush Mounted##OTHER##;Family Version##OTHER##;Interior Fitting##OTHER##;ETIM Article Class##OTHER##;EMCS Version##OTHER##;Double Door##OTHER##;Offset##LENGTH##MILLIMETERS;Model##OTHER##;Manufacturer##OTHER##;Door Width 2##LENGTH##MILLIMETERS;Door Width##LENGTH##MILLIMETERS;Door Type##OTHER##;Door Opening Angle [degrees]##OTHER##;Description##OTHER##;Depth (mm)##LENGTH##MILLIMETERS;Degree of Protection##OTHER##;Default Elevation##LENGTH##MILLIMETERS;Custom##OTHER##;Copyright##OTHER##;Content Supplier URL##OTHER##;Connection Voltage##ELECTRICAL_POTENTIAL##VOLTS;CB-NL Class##OTHER##;Bottom Width##LENGTH##MILLIMETERS;Bottom Clearance##LENGTH##MILLIMETERS;Base Family Version##OTHER##;Back Wall Void Width##LENGTH##MILLIMETERS;Back Clearance##LENGTH##MILLIMETERS;Article Type##OTHER##;Article Description##OTHER##;Area of Application##OTHER##;Trim Frame Type##OTHER##;Class of Protection with Accessories##OTHER##;Rated Operational Voltage Ue [V] AC##OTHER##;Locking Type — Lock##OTHER##
A19D - IP54 108 modules 1400x300x215;276.8;300;;;Color RAL 9016;www.stabiplan.com;12.5;1;111.3;111.3;111.3;111.3;www.stabiplan.com;0;300;;108;0;0;0;300;2017;250;9016;Double insulated;ABB;3;9;1;9;Sheet steel;https://new.abb.com/products/2CPX052105R9999;2CPX052105R9999;DISTRIBUTION_PANEL;250;;DISTRIBUTIONBOARD;IfcElectricDistributionPoint;275;1375;202.5;1400;622;1;137.5;;;E6211;300;0;12.11;Pre-assembled for installation of metering-, modules, Combi-Sets, CombiLine-Module on EDF-mounting frame;EC000058;4;0;215;A19D - IP54 108 modules 1400x300x215;ABB;275;275;Metal door;120;A19D Wall Cabinet 1PW9R PC2 IP54;215;IP54;0;0;© Stabiplan International BV;www.MEPcontent.com;400;;249.82;500;12.11;277;60;A19D - IP54 108 modules 1400x300x215;A19D Wall Cabinet 1PW9R PC2 IP54;Internal use;E_Distribution Panel_MEPcontent_ABB_Trim Frame CR19-59_INT-EN_Shared : CR19;;;
A29D - IP54 216 modules 1400x550x215;526.8;550;;;Color RAL 9016;www.stabiplan.com;12.5;1;111.3;111.3;111.3;361.3;www.stabiplan.com;0;300;;216;0;0;0;550;2017;250;9016;Double insulated;ABB;3;9;2;9;Sheet steel;https://new.abb.com/products/2CPX052106R9999;2CPX052106R9999;DISTRIBUTION_PANEL;250;;DISTRIBUTIONBOARD;IfcElectricDistributionPoint;525;1375;202.5;1400;622;1;262.5;;;E6211;550;0;12.11;Pre-assembled for installation of metering-, modules, Combi-Sets, CombiLine-Module on EDF-mounting frame;EC000058;4;0;215;A29D - IP54 216 modules 1400x550x215;ABB;525;525;Metal door;120;A29D Wall Cabinet 2PW9R PC2 IP54;215;IP54;0;0;© Stabiplan International BV;www.MEPcontent.com;400;;249.82;500;12.11;527;60;A29D - IP54 216 modules 1400x550x215;A29D Wall Cabinet 2PW9R PC2 IP54;Internal use;E_Distribution Panel_MEPcontent_ABB_Trim Frame CR19-59_INT-EN_Shared : CR29;;;
A39D - IP54 324 modules 1400x800x215;776.8;800;;;Color RAL 9016;www.stabiplan.com;12.5;1;111.3;111.3;611.3;361.3;www.stabiplan.com;0;300;;324;0;0;0;550;2017;250;9016;Double insulated;ABB;3;9;3;9;Sheet steel;https://new.abb.com/products/2CPX052107R9999;2CPX052107R9999;DISTRIBUTION_PANEL;300;;DISTRIBUTIONBOARD;IfcElectricDistributionPoint;775;1375;202.5;1400;622;1;387.5;;;E6211;550;0;12.11;Pre-assembled for installation of metering-, modules, Combi-Sets, CombiLine-Module on EDF-mounting frame;EC000058;4;1;215;A39D - IP54 324 modules 1400x800x215;ABB;249.1;525.9;Metal door;120;A39D Wall Cabinet 3PW9R PC2 IP54;215;IP54;0;0;© Stabiplan International BV;www.MEPcontent.com;400;;249.82;500;12.11;777;60;A39D - IP54 324 modules 1400x800x215;A39D Wall Cabinet 3PW9R PC2 IP54;Internal use;E_Distribution Panel_MEPcontent_ABB_Trim Frame CR19-59_INT-EN_Shared : CR39;;;
A49D - IP54 432 modules 1400x1050x215;1026.8;1050;;;Color RAL 9016;www.stabiplan.com;12.5;1;111.3;861.3;611.3;361.3;www.stabiplan.com;0;300;;432;0;0;0;550;2017;250;9016;Double insulated;ABB;3;9;4;9;Sheet steel;https://new.abb.com/products/2CPX052108R9999;2CPX052108R9999;DISTRIBUTION_PANEL;550;;DISTRIBUTIONBOARD;IfcElectricDistributionPoint;1025;1375;202.5;1400;622;1;512.5;;;E6211;550;0;12.11;Pre-assembled for installation of metering-, modules, Combi-Sets, CombiLine-Module on EDF-mounting frame;EC000058;4;1;215;A49D - IP54 432 modules 1400x1050x215;ABB;499.1;525.9;Metal door;120;A49D Wall Cabinet 4PW9R PC2 IP54;215;IP54;0;0;© Stabiplan International BV;www.MEPcontent.com;400;;249.82;500;12.11;1027;60;A49D - IP54 432 modules 1400x1050x215;A49D Wall Cabinet 4PW9R PC2 IP54;Internal use;E_Distribution Panel_MEPcontent_ABB_Trim Frame CR19-59_INT-EN_Shared : CR49;;;
A59D - IP54 540 modules 1400x1300x215;1276.8;1300;;;Color RAL 9016;www.stabiplan.com;12.5;1;1111.3;861.3;611.3;361.3;www.stabiplan.com;0;300;;540;0;0;0;800;2017;250;9016;Double insulated;ABB;3;9;5;9;Sheet steel;https://new.abb.com/products/2CPX052109R9999;2CPX052109R9999;DISTRIBUTION_PANEL;550;;DISTRIBUTIONBOARD;IfcElectricDistributionPoint;1275;1375;202.5;1400;622;1;637.5;;;E6211;800;0;12.11;Pre-assembled for installation of metering-, modules, Combi-Sets, CombiLine-Module on EDF-mounting frame;EC000058;4;1;215;A59D - IP54 540 modules 1400x1300x215;ABB;499.1;775.9;Metal door;120;A59D Wall Cabinet 5PW9R PC2 IP54;215;IP54;0;0;© Stabiplan International BV;www.MEPcontent.com;400;;249.82;500;12.11;1277;60;A59D - IP54 540 modules 1400x1300x215;A59D Wall Cabinet 5PW9R PC2 IP54;Internal use;E_Distribution Panel_MEPcontent_ABB_Trim Frame CR19-59_INT-EN_Shared : CR59;;;
A59 - IP44 540 modules 1400x1300x215;1276.8;1300;;;Color RAL 9016;www.stabiplan.com;12.5;1;1111.3;861.3;611.3;361.3;www.stabiplan.com;0;300;;540;0;0;0;800;2017;250;9016;Double insulated;ABB;3;9;5;9;Sheet steel;https://new.abb.com/products/2CPX052044R9999;2CPX052044R9999;DISTRIBUTION_PANEL;550;;DISTRIBUTIONBOARD;IfcElectricDistributionPoint;1275;1375;202.5;1400;622;1;637.5;;;E6211;800;0;12.11;Pre-assembled for installation of metering-, modules, Combi-Sets, CombiLine-Module on EDF-mounting frame;EC000248;4;1;215;A59 - IP44 540 modules 1400x1300x215;ABB;499.1;775.9;Metal door;120;A59 Wall Cabinet 5PW9R PC2 IP44;215;IP44;0;0;© Stabiplan International BV;www.MEPcontent.com;400;;249.82;500;12.11;1277;60;A59 - IP44 540 modules 1400x1300x215;A59 Wall Cabinet 5PW9R PC2 IP44;Internal use;E_Distribution Panel_MEPcontent_ABB_Trim Frame CR19-59_INT-EN_Shared : CR59;;;
A49 - IP44 432 modules 1400x1050x215;1026.8;1050;;;Color RAL 9016;www.stabiplan.com;12.5;1;111.3;861.3;611.3;361.3;www.stabiplan.com;0;300;;432;0;0;0;550;2017;250;9016;Double insulated;ABB;3;9;4;9;Sheet steel;https://new.abb.com/products/2CPX052043R9999;2CPX052043R9999;DISTRIBUTION_PANEL;550;;DISTRIBUTIONBOARD;IfcElectricDistributionPoint;1025;1375;202.5;1400;622;1;512.5;;;E6211;550;0;12.11;Pre-assembled for installation of metering-, modules, Combi-Sets, CombiLine-Module on EDF-mounting frame;EC000248;4;1;215;A49 - IP44 432 modules 1400x1050x215;ABB;499.1;525.9;Metal door;120;A49 Wall Cabinet 4PW9R PC2 IP44;215;IP44;0;0;© Stabiplan International BV;www.MEPcontent.com;400;;249.82;500;12.11;1027;60;A49 - IP44 432 modules 1400x1050x215;A49 Wall Cabinet 4PW9R PC2 IP44;Internal use;E_Distribution Panel_MEPcontent_ABB_Trim Frame CR19-59_INT-EN_Shared : CR49;;;
A39 - IP44 324 modules 1400x800x215;776.8;800;;;Color RAL 9016;www.stabiplan.com;12.5;1;111.3;111.3;611.3;361.3;www.stabiplan.com;0;300;;324;0;0;0;550;2017;250;9016;Double insulated;ABB;3;9;3;9;Sheet steel;https://new.abb.com/products/2CPX052042R9999;2CPX052042R9999;DISTRIBUTION_PANEL;300;;DISTRIBUTIONBOARD;IfcElectricDistributionPoint;775;1375;202.5;1400;622;1;387.5;;;E6211;550;0;12.11;Pre-assembled for installation of metering-, modules, Combi-Sets, CombiLine-Module on EDF-mounting frame;EC000248;4;1;215;A39 - IP44 324 modules 1400x800x215;ABB;249.1;525.9;Metal door;120;A39 Wall Cabinet 3PW9R PC2 IP44;215;IP44;0;0;© Stabiplan International BV;www.MEPcontent.com;400;;249.82;500;12.11;777;60;A39 - IP44 324 modules 1400x800x215;A39 Wall Cabinet 3PW9R PC2 IP44;Internal use;E_Distribution Panel_MEPcontent_ABB_Trim Frame CR19-59_INT-EN_Shared : CR39;;;
A29 - IP44 216 modules 1400x550x215;526.8;550;;;Color RAL 9016;www.stabiplan.com;12.5;1;111.3;111.3;111.3;361.3;www.stabiplan.com;0;300;;216;0;0;0;550;2017;250;9016;Double insulated;ABB;3;9;2;9;Sheet steel;https://new.abb.com/products/2CPX052041R9999;2CPX052041R9999;DISTRIBUTION_PANEL;250;;DISTRIBUTIONBOARD;IfcElectricDistributionPoint;525;1375;202.5;1400;622;1;262.5;;;E6211;550;0;12.11;Pre-assembled for installation of metering-, modules, Combi-Sets, CombiLine-Module on EDF-mounting frame;EC000248;4;0;215;A29 - IP44 216 modules 1400x550x215;ABB;525;525;Metal door;120;A29 Wall Cabinet 2PW9R PC2 IP44;215;IP44;0;0;© Stabiplan International BV;www.MEPcontent.com;400;;249.82;500;12.11;527;60;A29 - IP44 216 modules 1400x550x215;A29 Wall Cabinet 2PW9R PC2 IP44;Internal use;E_Distribution Panel_MEPcontent_ABB_Trim Frame CR19-59_INT-EN_Shared : CR29;;;
A19 - IP44 108 modules 1400x300x215;276.8;300;;;Color RAL 9016;www.stabiplan.com;12.5;1;111.3;111.3;111.3;111.3;www.stabiplan.com;0;300;;108;0;0;0;300;2017;250;9016;Double insulated;ABB;3;9;1;9;Sheet steel;https://new.abb.com/products/2CPX052040R9999;2CPX052040R9999;DISTRIBUTION_PANEL;250;;DISTRIBUTIONBOARD;IfcElectricDistributionPoint;275;1375;202.5;1400;622;1;137.5;;;E6211;300;0;12.11;Pre-assembled for installation of metering-, modules, Combi-Sets, CombiLine-Module on EDF-mounting frame;EC000248;4;0;215;A19 - IP44 108 modules 1400x300x215;ABB;275;275;Metal door;120;A19 Wall Cabinet 1PW9R PC2 IP44;215;IP44;0;0;© Stabiplan International BV;www.MEPcontent.com;400;;249.82;500;12.11;277;60;A19 - IP44 108 modules 1400x300x215;A19 Wall Cabinet 1PW9R PC2 IP44;Internal use;E_Distribution Panel_MEPcontent_ABB_Trim Frame CR19-59_INT-EN_Shared : CR19;;;
