;Width Safe##LENGTH##MILLIMETERS;Width (mm)##LENGTH##MILLIMETERS;Wholesaler Art. No.##OTHER##;Wholesaler##OTHER##;White##OTHER##;Watermarked By##OTHER##;Wall Thickness##LENGTH##MILLIMETERS;Wall Mounted##OTHER##;Upper Width 4##LENGTH##MILLIMETERS;Upper Width 3##LENGTH##MILLIMETERS;Upper Width 2##LENGTH##MILLIMETERS;Upper Width 1##LENGTH##MILLIMETERS;URL##OTHER##;Trim Frame Visible##OTHER##;Top Clearance##LENGTH##MILLIMETERS;Symbol ID##OTHER##;Stabu Code##OTHER##;Space Units [SU]##OTHER##;Show Service Space Safe##OTHER##;Show Service Area Inside Wall##OTHER##;Show Service Area##OTHER##;Rotation W-Axis Default Correction##ANGLE##DEGREES;Rotation V-Axis Default Correction##ANGLE##DEGREES;Rotation U-Axis Default Correction##ANGLE##DEGREES;Right Door##OTHER##;Right Clearance##LENGTH##MILLIMETERS;Revit Version##OTHER##;Rated Operational Voltage Ue [V] AC##OTHER##;Rated Current In [A]##OTHER##;RAL-Number##OTHER##;Protection Class##OTHER##;Product Line##OTHER##;Phase##OTHER##;Panel Width (PW)##OTHER##;Number of Rows##OTHER##;Material of Enclosures##OTHER##;Manufacturer URL##OTHER##;Manufacturer Art. No.##OTHER##;MEPcontent Class##OTHER##;Locking Type — Lock##OTHER##;Left Door##OTHER##;Left Clearance##LENGTH##MILLIMETERS;Internal Art. No.##OTHER##;Interior Fitting##OTHER##;IFCExportType##OTHER##;IFCExportAs##OTHER##;Hole Width##LENGTH##MILLIMETERS;Hole Height##LENGTH##MILLIMETERS;Hole Depth##LENGTH##MILLIMETERS;Height (mm)##LENGTH##MILLIMETERS;Handle Height##LENGTH##MILLIMETERS;Handle##OTHER##;Door##OTHER##;Half Width##LENGTH##MILLIMETERS;Grid Units (GU)##OTHER##;GTIN##OTHER##;GLN##OTHER##;Function Code##OTHER##;Front Clearance##LENGTH##MILLIMETERS;Flush Mounted##OTHER##;Family Version##OTHER##;ETIM Article Class##OTHER##;EMCS Version##OTHER##;Double Door##OTHER##;Offset##LENGTH##MILLIMETERS;Model##OTHER##;Manufacturer##OTHER##;Door Width 2##LENGTH##MILLIMETERS;Door Width##LENGTH##MILLIMETERS;Door Type##OTHER##;Door Opening Angle [degrees]##OTHER##;Description##OTHER##;Depth (mm)##LENGTH##MILLIMETERS;Degree of Protection##OTHER##;Default Elevation##LENGTH##MILLIMETERS;Custom##OTHER##;Copyright##OTHER##;Content Supplier URL##OTHER##;Connection Voltage##ELECTRICAL_POTENTIAL##VOLTS;Class of Protection with Accessories##OTHER##;Category##OTHER##;CB-NL Class##OTHER##;Bottom Width##LENGTH##MILLIMETERS;Bottom Clearance##LENGTH##MILLIMETERS;Base Family Version##OTHER##;Back Wall Void Width##LENGTH##MILLIMETERS;Back Clearance##LENGTH##MILLIMETERS;Article Type##OTHER##;Article Description##OTHER##;Article Code##OTHER##;Area of Application##OTHER##;App ID##OTHER##;Right Door Type##OTHER##;Left Door Type##OTHER##;Trim Frame Type##OTHER##
A19B - 108 modules 1400x300x215 empty without door;276.8;300;;;Color RAL 9016;www.stabiplan.com;12.5;1;111.3;111.3;111.3;111.3;www.stabiplan.com;0;300;UNKNOWN;;108;0;0;0;0;0;0;1;300;2017;400;125;9016;Double insulated;ABB;3;1;;Sheet steel;https://new.abb.com/products/2CPX052088R9999;2CPX052088R9999;DISTRIBUTION_PANEL;;0;250;;Pre-assembled for installation of modules and CombiLine Modules;DISTRIBUTIONBOARD;IfcElectricDistributionPoint;275;1375;202.5;1400;617.5;1;0;137.5;9;;;;300;0;12.11;EC000058;4;0;215;A19B - 108 modules 1400x300x215 empty without door;ABB;275;275;Without door;;A19B Wall Cab.1PW9R basic empty without door;215;IP30;0;0;© Stabiplan International BV;www.MEPcontent.com;400;In combination with earthing set (accessory) we can achieve protection class 1;EL_PANEL;;249.82;500;12.11;277;60;A19B - 108 modules 1400x300x215 empty without door;A19B Wall Cab.1PW9R basic empty without door;;Internal use;EL_MODELPARTSYSTEM_MC;E_Distribution Panel_MEPcontent_ABB_Right Door_INT-EN_Shared : CTB19S;E_Distribution Panel_MEPcontent_ABB_Left Door_INT-EN_Shared : CTB19;E_Distribution Panel_MEPcontent_ABB_Trim Frame CR19-59_INT-EN_Shared : CR19
A19B - 108 modules 1400x300x215 transparent door;276.8;300;;;Color RAL 9016;www.stabiplan.com;12.5;1;111.3;111.3;111.3;111.3;www.stabiplan.com;0;300;UNKNOWN;;108;0;0;0;0;0;0;1;300;2017;400;125;9016;Double insulated;ABB;3;1;;Sheet steel;https://new.abb.com/products/2CPX052088R9999;2CPX052088R9999;DISTRIBUTION_PANEL;;0;250;;Pre-assembled for installation of modules and CombiLine Modules;DISTRIBUTIONBOARD;IfcElectricDistributionPoint;275;1375;202.5;1400;617.5;1;1;137.5;9;;;;300;0;12.11;EC000058;4;0;215;A19B - 108 modules 1400x300x215 transparent door;ABB;275;275;Transparent door;120;A19B Wall Cab.1PW9R basic transparent door;215;IP44;0;0;© Stabiplan International BV;www.MEPcontent.com;400;In combination with earthing set (accessory) we can achieve protection class 1;EL_PANEL;;249.82;500;12.11;277;60;A19B - 108 modules 1400x300x215 transparent door;A19B Wall Cab.1PW9R basic transparent door;;Internal use;EL_MODELPARTSYSTEM_MC;E_Distribution Panel_MEPcontent_ABB_Right Door_INT-EN_Shared : CTT19S;E_Distribution Panel_MEPcontent_ABB_Left Door_INT-EN_Shared : CTB19;E_Distribution Panel_MEPcontent_ABB_Trim Frame CR19-59_INT-EN_Shared : CR19
A19B - 108 modules 1400x300x215 media ventilated;276.8;300;;;Color RAL 9016;www.stabiplan.com;12.5;1;111.3;111.3;111.3;111.3;www.stabiplan.com;0;300;UNKNOWN;;108;0;0;0;0;0;0;1;300;2017;400;125;9016;Double insulated;ABB;3;1;;Sheet steel;https://new.abb.com/products/2CPX052088R9999;2CPX052088R9999;DISTRIBUTION_PANEL;;0;250;;Pre-assembled for installation of modules and CombiLine Modules;DISTRIBUTIONBOARD;IfcElectricDistributionPoint;275;1375;202.5;1400;617.5;1;1;137.5;9;;;;300;0;12.11;EC000058;4;0;215;A19B - 108 modules 1400x300x215 media ventilated;ABB;275;275;Ventilated metal door;120;A19B Wall Cab.1PW9R basic media ventilaton;215;IP44;0;0;© Stabiplan International BV;www.MEPcontent.com;400;In combination with earthing set (accessory) we can achieve protection class 1;EL_PANEL;;249.82;500;12.11;277;60;A19B - 108 modules 1400x300x215 media ventilated;A19B Wall Cab.1PW9R basic media ventilaton;;Internal use;EL_MODELPARTSYSTEM_MC;E_Distribution Panel_MEPcontent_ABB_Right Door_INT-EN_Shared : CTL19S;E_Distribution Panel_MEPcontent_ABB_Left Door_INT-EN_Shared : CTB19;E_Distribution Panel_MEPcontent_ABB_Trim Frame CR19-59_INT-EN_Shared : CR19
A19B - 108 modules 1400x300x215 media WiFi;276.8;300;;;Color RAL 9016;www.stabiplan.com;12.5;1;111.3;111.3;111.3;111.3;www.stabiplan.com;0;300;UNKNOWN;;108;0;0;0;0;0;0;1;300;2017;400;125;9016;Double insulated;ABB;3;1;;Sheet steel;https://new.abb.com/products/2CPX052088R9999;2CPX052088R9999;DISTRIBUTION_PANEL;;0;250;;Pre-assembled for installation of modules and CombiLine Modules;DISTRIBUTIONBOARD;IfcElectricDistributionPoint;275;1375;202.5;1400;617.5;1;1;137.5;9;;;;300;0;12.11;EC000058;4;0;215;A19B - 108 modules 1400x300x215 media WiFi;ABB;275;275;Ventilated metal door WiFi;120;A19B Wall Cab.1PW9R basic media WiFi;215;IP44;0;0;© Stabiplan International BV;www.MEPcontent.com;400;In combination with earthing set (accessory) we can achieve protection class 1;EL_PANEL;;249.82;500;12.11;277;60;A19B - 108 modules 1400x300x215 media WiFi;A19B Wall Cab.1PW9R basic media WiFi;;Internal use;EL_MODELPARTSYSTEM_MC;E_Distribution Panel_MEPcontent_ABB_Right Door_INT-EN_Shared : CTW19S;E_Distribution Panel_MEPcontent_ABB_Left Door_INT-EN_Shared : CTB19;E_Distribution Panel_MEPcontent_ABB_Trim Frame CR19-59_INT-EN_Shared : CR19
A19B - 108 modules 1400x300x215 empty with door;276.8;300;;;Color RAL 9016;www.stabiplan.com;12.5;1;111.3;111.3;111.3;111.3;www.stabiplan.com;0;300;UNKNOWN;;108;0;0;0;0;0;0;1;300;2017;400;125;9016;Double insulated;ABB;3;1;;Sheet steel;https://new.abb.com/products/2CPX052088R9999;2CPX052088R9999;DISTRIBUTION_PANEL;;0;250;;Pre-assembled for installation of modules and CombiLine Modules;DISTRIBUTIONBOARD;IfcElectricDistributionPoint;275;1375;202.5;1400;617.5;1;1;137.5;9;;;;300;0;12.11;EC000058;4;0;215;A19B - 108 modules 1400x300x215 empty with door;ABB;275;275;Metal door;120;A19B Wall Cab.1PW9R basic empty with door;215;IP44;0;0;© Stabiplan International BV;www.MEPcontent.com;400;In combination with earthing set (accessory) we can achieve protection class 1;EL_PANEL;;249.82;500;12.11;277;60;A19B - 108 modules 1400x300x215 empty with door;A19B Wall Cab.1PW9R basic empty with door;;Internal use;EL_MODELPARTSYSTEM_MC;E_Distribution Panel_MEPcontent_ABB_Right Door_INT-EN_Shared : CTB19S;E_Distribution Panel_MEPcontent_ABB_Left Door_INT-EN_Shared : CTB19;E_Distribution Panel_MEPcontent_ABB_Trim Frame CR19-59_INT-EN_Shared : CR19
A29B - 216 modules 1400x550x215 empty without door;526.8;550;;;Color RAL 9016;www.stabiplan.com;12.5;1;111.3;111.3;111.3;111.3;www.stabiplan.com;0;300;UNKNOWN;;216;0;0;0;0;0;0;1;550;2017;400;125;9016;Double insulated;ABB;3;2;;Sheet steel;https://new.abb.com/products/2CPX052089R9999;2CPX052089R9999;DISTRIBUTION_PANEL;;0;250;;Pre-assembled for installation of modules and CombiLine Modules;DISTRIBUTIONBOARD;IfcElectricDistributionPoint;525;1375;202.5;1400;617.5;1;0;262.5;9;;;;550;0;12.11;EC000058;4;0;215;A29B - 216 modules 1400x550x215 empty without door;ABB;525;525;Without door;;A29B Wall Cab.2PW9R basic empty without door;215;IP30;0;0;© Stabiplan International BV;www.MEPcontent.com;400;In combination with earthing set (accessory) we can achieve protection class 1;EL_PANEL;;249.82;500;12.11;527;60;A29B - 216 modules 1400x550x215 empty without door;A29B Wall Cab.2PW9R basic empty without door;;Internal use;EL_MODELPARTSYSTEM_MC;E_Distribution Panel_MEPcontent_ABB_Right Door_INT-EN_Shared : CTB29S;E_Distribution Panel_MEPcontent_ABB_Left Door_INT-EN_Shared : CTB19;E_Distribution Panel_MEPcontent_ABB_Trim Frame CR19-59_INT-EN_Shared : CR29
A29B - 216 modules 1400x550x215 transparent door;526.8;550;;;Color RAL 9016;www.stabiplan.com;12.5;1;111.3;111.3;111.3;111.3;www.stabiplan.com;0;300;UNKNOWN;;216;0;0;0;0;0;0;1;550;2017;400;125;9016;Double insulated;ABB;3;2;;Sheet steel;https://new.abb.com/products/2CPX052089R9999;2CPX052089R9999;DISTRIBUTION_PANEL;;0;250;;Pre-assembled for installation of modules and CombiLine Modules;DISTRIBUTIONBOARD;IfcElectricDistributionPoint;525;1375;202.5;1400;617.5;1;1;262.5;9;;;;550;0;12.11;EC000058;4;0;215;A29B - 216 modules 1400x550x215 transparent door;ABB;525;525;Transparent door;120;A29B Wall Cab.2PW9R basic transparent door;215;IP44;0;0;© Stabiplan International BV;www.MEPcontent.com;400;In combination with earthing set (accessory) we can achieve protection class 1;EL_PANEL;;249.82;500;12.11;527;60;A29B - 216 modules 1400x550x215 transparent door;A29B Wall Cab.2PW9R basic transparent door;;Internal use;EL_MODELPARTSYSTEM_MC;E_Distribution Panel_MEPcontent_ABB_Right Door_INT-EN_Shared : CTT29S;E_Distribution Panel_MEPcontent_ABB_Left Door_INT-EN_Shared : CTB19;E_Distribution Panel_MEPcontent_ABB_Trim Frame CR19-59_INT-EN_Shared : CR29
A29B - 216 modules 1400x550x215 media ventilated;526.8;550;;;Color RAL 9016;www.stabiplan.com;12.5;1;111.3;111.3;111.3;111.3;www.stabiplan.com;0;300;UNKNOWN;;216;0;0;0;0;0;0;1;550;2017;400;125;9016;Double insulated;ABB;3;2;;Sheet steel;https://new.abb.com/products/2CPX052089R9999;2CPX052089R9999;DISTRIBUTION_PANEL;;0;250;;Pre-assembled for installation of modules and CombiLine Modules;DISTRIBUTIONBOARD;IfcElectricDistributionPoint;525;1375;202.5;1400;617.5;1;1;262.5;9;;;;550;0;12.11;EC000058;4;0;215;A29B - 216 modules 1400x550x215 media ventilated;ABB;525;525;Ventilated metal door;120;A29B Wall Cab.2PW9R basic media ventilated;215;IP44;0;0;© Stabiplan International BV;www.MEPcontent.com;400;In combination with earthing set (accessory) we can achieve protection class 1;EL_PANEL;;249.82;500;12.11;527;60;A29B - 216 modules 1400x550x215 media ventilated;A29B Wall Cab.2PW9R basic media ventilated;;Internal use;EL_MODELPARTSYSTEM_MC;E_Distribution Panel_MEPcontent_ABB_Right Door_INT-EN_Shared : CTL29S;E_Distribution Panel_MEPcontent_ABB_Left Door_INT-EN_Shared : CTB19;E_Distribution Panel_MEPcontent_ABB_Trim Frame CR19-59_INT-EN_Shared : CR29
A29B - 216 modules 1400x550x215 media WiFi;526.8;550;;;Color RAL 9016;www.stabiplan.com;12.5;1;111.3;111.3;111.3;111.3;www.stabiplan.com;0;300;UNKNOWN;;216;0;0;0;0;0;0;1;550;2017;400;125;9016;Double insulated;ABB;3;2;;Sheet steel;https://new.abb.com/products/2CPX052089R9999;2CPX052089R9999;DISTRIBUTION_PANEL;;0;250;;Pre-assembled for installation of modules and CombiLine Modules;DISTRIBUTIONBOARD;IfcElectricDistributionPoint;525;1375;202.5;1400;617.5;1;1;262.5;9;;;;550;0;12.11;EC000058;4;0;215;A29B - 216 modules 1400x550x215 media WiFi;ABB;525;525;Ventilated metal door WiFi;120;A29B Wall Cab.2PW9R basic media WiFi;215;IP44;0;0;© Stabiplan International BV;www.MEPcontent.com;400;In combination with earthing set (accessory) we can achieve protection class 1;EL_PANEL;;249.82;500;12.11;527;60;A29B - 216 modules 1400x550x215 media WiFi;A29B Wall Cab.2PW9R basic media WiFi;;Internal use;EL_MODELPARTSYSTEM_MC;E_Distribution Panel_MEPcontent_ABB_Right Door_INT-EN_Shared : CTW29S;E_Distribution Panel_MEPcontent_ABB_Left Door_INT-EN_Shared : CTB19;E_Distribution Panel_MEPcontent_ABB_Trim Frame CR19-59_INT-EN_Shared : CR29
A29B - 216 modules 1400x550x215 empty with door;526.8;550;;;Color RAL 9016;www.stabiplan.com;12.5;1;111.3;111.3;111.3;111.3;www.stabiplan.com;0;300;UNKNOWN;;216;0;0;0;0;0;0;1;550;2017;400;125;9016;Double insulated;ABB;3;2;;Sheet steel;https://new.abb.com/products/2CPX052089R9999;2CPX052089R9999;DISTRIBUTION_PANEL;;0;250;;Pre-assembled for installation of modules and CombiLine Modules;DISTRIBUTIONBOARD;IfcElectricDistributionPoint;525;1375;202.5;1400;617.5;1;1;262.5;9;;;;550;0;12.11;EC000058;4;0;215;A29B - 216 modules 1400x550x215 empty with door;ABB;525;525;Metal door;120;A29B Wall Cab.2PW9R basic empty with door;215;IP44;0;0;© Stabiplan International BV;www.MEPcontent.com;400;In combination with earthing set (accessory) we can achieve protection class 1;EL_PANEL;;249.82;500;12.11;527;60;A29B - 216 modules 1400x550x215 empty with door;A29B Wall Cab.2PW9R basic empty with door;;Internal use;EL_MODELPARTSYSTEM_MC;E_Distribution Panel_MEPcontent_ABB_Right Door_INT-EN_Shared : CTB29S;E_Distribution Panel_MEPcontent_ABB_Left Door_INT-EN_Shared : CTB19;E_Distribution Panel_MEPcontent_ABB_Trim Frame CR19-59_INT-EN_Shared : CR29
A39B - 324 modules 1400x800x215 empty without door;776.8;800;;;Color RAL 9016;www.stabiplan.com;12.5;1;111.3;111.3;111.3;111.3;www.stabiplan.com;0;300;UNKNOWN;;324;0;0;0;0;0;0;1;550;2017;400;125;9016;Double insulated;ABB;3;3;;Sheet steel;https://new.abb.com/products/2CPX052090R9999;2CPX052090R9999;DISTRIBUTION_PANEL;;1;300;;Pre-assembled for installation of modules and CombiLine Modules;DISTRIBUTIONBOARD;IfcElectricDistributionPoint;775;1375;202.5;1400;617.5;1;0;387.5;9;;;;550;0;12.11;EC000058;4;0;215;A39B - 324 modules 1400x800x215 empty without door;ABB;249.1;775;Without door;;A39B Wall Cab.3PW9R basic empty without door;215;IP30;0;0;© Stabiplan International BV;www.MEPcontent.com;400;In combination with earthing set (accessory) we can achieve protection class 1;EL_PANEL;;249.82;500;12.11;777;60;A39B - 324 modules 1400x800x215 empty without door;A39B Wall Cab.3PW9R basic empty without door;;Internal use;EL_MODELPARTSYSTEM_MC;E_Distribution Panel_MEPcontent_ABB_Right Door_INT-EN_Shared : CTB29S;E_Distribution Panel_MEPcontent_ABB_Left Door_INT-EN_Shared : CTB19;E_Distribution Panel_MEPcontent_ABB_Trim Frame CR19-59_INT-EN_Shared : CR39
A39B - 324 modules 1400x800x215 transparent door;776.8;800;;;Color RAL 9016;www.stabiplan.com;12.5;1;111.3;111.3;111.3;111.3;www.stabiplan.com;0;300;UNKNOWN;;324;0;0;0;0;0;0;1;550;2017;400;125;9016;Double insulated;ABB;3;3;;Sheet steel;https://new.abb.com/products/2CPX052090R9999;2CPX052090R9999;DISTRIBUTION_PANEL;;1;300;;Pre-assembled for installation of modules and CombiLine Modules;DISTRIBUTIONBOARD;IfcElectricDistributionPoint;775;1375;202.5;1400;617.5;1;1;387.5;9;;;;550;0;12.11;EC000058;4;1;215;A39B - 324 modules 1400x800x215 transparent door;ABB;249.1;775;Transparent door;120;A39B Wall Cab.3PW9R basic transparent door;215;IP44;0;0;© Stabiplan International BV;www.MEPcontent.com;400;In combination with earthing set (accessory) we can achieve protection class 1;EL_PANEL;;249.82;500;12.11;777;60;A39B - 324 modules 1400x800x215 transparent door;A39B Wall Cab.3PW9R basic transparent door;;Internal use;EL_MODELPARTSYSTEM_MC;E_Distribution Panel_MEPcontent_ABB_Right Door_INT-EN_Shared : CTT29S;E_Distribution Panel_MEPcontent_ABB_Left Door_INT-EN_Shared : CTT19;E_Distribution Panel_MEPcontent_ABB_Trim Frame CR19-59_INT-EN_Shared : CR39
A39B - 324 modules 1400x800x215 media ventilated;776.8;800;;;Color RAL 9016;www.stabiplan.com;12.5;1;111.3;111.3;111.3;111.3;www.stabiplan.com;0;300;UNKNOWN;;324;0;0;0;0;0;0;1;550;2017;400;125;9016;Double insulated;ABB;3;3;;Sheet steel;https://new.abb.com/products/2CPX052090R9999;2CPX052090R9999;DISTRIBUTION_PANEL;;1;300;;Pre-assembled for installation of modules and CombiLine Modules;DISTRIBUTIONBOARD;IfcElectricDistributionPoint;775;1375;202.5;1400;617.5;1;1;387.5;9;;;;550;0;12.11;EC000058;4;1;215;A39B - 324 modules 1400x800x215 media ventilated;ABB;249.1;775;Ventilated metal door;120;A39B Wall Cab.3PW9R basic media ventilated;215;IP44;0;0;© Stabiplan International BV;www.MEPcontent.com;400;In combination with earthing set (accessory) we can achieve protection class 1;EL_PANEL;;249.82;500;12.11;777;60;A39B - 324 modules 1400x800x215 media ventilated;A39B Wall Cab.3PW9R basic media ventilated;;Internal use;EL_MODELPARTSYSTEM_MC;E_Distribution Panel_MEPcontent_ABB_Right Door_INT-EN_Shared : CTL29S;E_Distribution Panel_MEPcontent_ABB_Left Door_INT-EN_Shared : CTB19;E_Distribution Panel_MEPcontent_ABB_Trim Frame CR19-59_INT-EN_Shared : CR39
A39B - 324 modules 1400x800x215 media WiFi;776.8;800;;;Color RAL 9016;www.stabiplan.com;12.5;1;111.3;111.3;111.3;111.3;www.stabiplan.com;0;300;UNKNOWN;;324;0;0;0;0;0;0;1;550;2017;400;125;9016;Double insulated;ABB;3;3;;Sheet steel;https://new.abb.com/products/2CPX052090R9999;2CPX052090R9999;DISTRIBUTION_PANEL;;1;300;;Pre-assembled for installation of modules and CombiLine Modules;DISTRIBUTIONBOARD;IfcElectricDistributionPoint;775;1375;202.5;1400;617.5;1;1;387.5;9;;;;550;0;12.11;EC000058;4;1;215;A39B - 324 modules 1400x800x215 media WiFi;ABB;249.1;775;Ventilated metal door WiFi;120;A39B Wall Cab.3PW9R basic media WiFi;215;IP44;0;0;© Stabiplan International BV;www.MEPcontent.com;400;In combination with earthing set (accessory) we can achieve protection class 1;EL_PANEL;;249.82;500;12.11;777;60;A39B - 324 modules 1400x800x215 media WiFi;A39B Wall Cab.3PW9R basic media WiFi;;Internal use;EL_MODELPARTSYSTEM_MC;E_Distribution Panel_MEPcontent_ABB_Right Door_INT-EN_Shared : CTW29S;E_Distribution Panel_MEPcontent_ABB_Left Door_INT-EN_Shared : CTB19;E_Distribution Panel_MEPcontent_ABB_Trim Frame CR19-59_INT-EN_Shared : CR39
A39B - 324 modules 1400x800x215 empty with door;776.8;800;;;Color RAL 9016;www.stabiplan.com;12.5;1;111.3;111.3;111.3;111.3;www.stabiplan.com;0;300;UNKNOWN;;324;0;0;0;0;0;0;1;550;2017;400;125;9016;Double insulated;ABB;3;3;;Sheet steel;https://new.abb.com/products/2CPX052090R9999;2CPX052090R9999;DISTRIBUTION_PANEL;;1;300;;Pre-assembled for installation of modules and CombiLine Modules;DISTRIBUTIONBOARD;IfcElectricDistributionPoint;775;1375;202.5;1400;617.5;1;1;387.5;9;;;;550;0;12.11;EC000058;4;1;215;A39B - 324 modules 1400x800x215 empty with door;ABB;249.1;775;Metal door;120;A39B Wall Cab.3PW9R basic empty with door;215;IP44;0;0;© Stabiplan International BV;www.MEPcontent.com;400;In combination with earthing set (accessory) we can achieve protection class 1;EL_PANEL;;249.82;500;12.11;777;60;A39B - 324 modules 1400x800x215 empty with door;A39B Wall Cab.3PW9R basic empty with door;;Internal use;EL_MODELPARTSYSTEM_MC;E_Distribution Panel_MEPcontent_ABB_Right Door_INT-EN_Shared : CTB29S;E_Distribution Panel_MEPcontent_ABB_Left Door_INT-EN_Shared : CTB19;E_Distribution Panel_MEPcontent_ABB_Trim Frame CR19-59_INT-EN_Shared : CR39
A49B - 432 modules 1400x1050x215 empty without door;1026.8;1050;;;Color RAL 9016;www.stabiplan.com;12.5;1;111.3;111.3;111.3;111.3;www.stabiplan.com;0;300;UNKNOWN;;432;0;0;0;0;0;0;1;550;2017;400;125;9016;Double insulated;ABB;3;4;;Sheet steel;https://new.abb.com/products/2CPX052091R9999;2CPX052091R9999;DISTRIBUTION_PANEL;;1;550;;Pre-assembled for installation of modules and CombiLine Modules;DISTRIBUTIONBOARD;IfcElectricDistributionPoint;1025;1375;202.5;1400;617.5;1;0;512.5;9;;;;550;0;12.11;EC000058;4;0;215;A49B - 432 modules 1400x1050x215 empty without door;ABB;499.1;1025;Without door;;A49B Wall Cab.4PW9R basic empty without door;215;IP30;0;0;© Stabiplan International BV;www.MEPcontent.com;400;In combination with earthing set (accessory) we can achieve protection class 1;EL_PANEL;;249.82;500;12.11;1027;60;A49B - 432 modules 1400x1050x215 empty without door;A49B Wall Cab.4PW9R basic empty without door;;Internal use;EL_MODELPARTSYSTEM_MC;E_Distribution Panel_MEPcontent_ABB_Right Door_INT-EN_Shared : CTB29S;E_Distribution Panel_MEPcontent_ABB_Left Door_INT-EN_Shared : CTB29;E_Distribution Panel_MEPcontent_ABB_Trim Frame CR19-59_INT-EN_Shared : CR49
A49B - 432 modules 1400x1050x215 transparent door;1026.8;1050;;;Color RAL 9016;www.stabiplan.com;12.5;1;111.3;111.3;111.3;111.3;www.stabiplan.com;0;300;UNKNOWN;;432;0;0;0;0;0;0;1;550;2017;400;125;9016;Double insulated;ABB;3;4;;Sheet steel;https://new.abb.com/products/2CPX052091R9999;2CPX052091R9999;DISTRIBUTION_PANEL;;1;550;;Pre-assembled for installation of modules and CombiLine Modules;DISTRIBUTIONBOARD;IfcElectricDistributionPoint;1025;1375;202.5;1400;617.5;1;1;512.5;9;;;;550;0;12.11;EC000058;4;1;215;A49B - 432 modules 1400x1050x215 transparent door;ABB;499.1;1025;Transparent door;120;A49B Wall Cab.4PW9R basic transparent door;215;IP44;0;0;© Stabiplan International BV;www.MEPcontent.com;400;In combination with earthing set (accessory) we can achieve protection class 1;EL_PANEL;;249.82;500;12.11;1027;60;A49B - 432 modules 1400x1050x215 transparent door;A49B Wall Cab.4PW9R basic transparent door;;Internal use;EL_MODELPARTSYSTEM_MC;E_Distribution Panel_MEPcontent_ABB_Right Door_INT-EN_Shared : CTT29S;E_Distribution Panel_MEPcontent_ABB_Left Door_INT-EN_Shared : CTT29;E_Distribution Panel_MEPcontent_ABB_Trim Frame CR19-59_INT-EN_Shared : CR49
A49B - 432 modules 1400x1050x215 media ventilated;1026.8;1050;;;Color RAL 9016;www.stabiplan.com;12.5;1;111.3;111.3;111.3;111.3;www.stabiplan.com;0;300;UNKNOWN;;432;0;0;0;0;0;0;1;550;2017;400;125;9016;Double insulated;ABB;3;4;;Sheet steel;https://new.abb.com/products/2CPX052091R9999;2CPX052091R9999;DISTRIBUTION_PANEL;;1;550;;Pre-assembled for installation of modules and CombiLine Modules;DISTRIBUTIONBOARD;IfcElectricDistributionPoint;1025;1375;202.5;1400;617.5;1;1;512.5;9;;;;550;0;12.11;EC000058;4;1;215;A49B - 432 modules 1400x1050x215 media ventilated;ABB;499.1;1025;Ventilated metal door;120;A49B Wall Cab.4PW9R basic media ventilated;215;IP44;0;0;© Stabiplan International BV;www.MEPcontent.com;400;In combination with earthing set (accessory) we can achieve protection class 1;EL_PANEL;;249.82;500;12.11;1027;60;A49B - 432 modules 1400x1050x215 media ventilated;A49B Wall Cab.4PW9R basic media ventilated;;Internal use;EL_MODELPARTSYSTEM_MC;E_Distribution Panel_MEPcontent_ABB_Right Door_INT-EN_Shared : CTL29S;E_Distribution Panel_MEPcontent_ABB_Left Door_INT-EN_Shared : CTB29;E_Distribution Panel_MEPcontent_ABB_Trim Frame CR19-59_INT-EN_Shared : CR49
A49B - 432 modules 1400x1050x215 media WiFi;1026.8;1050;;;Color RAL 9016;www.stabiplan.com;12.5;1;111.3;111.3;111.3;111.3;www.stabiplan.com;0;300;UNKNOWN;;432;0;0;0;0;0;0;1;550;2017;400;125;9016;Double insulated;ABB;3;4;;Sheet steel;https://new.abb.com/products/2CPX052091R9999;2CPX052091R9999;DISTRIBUTION_PANEL;;1;550;;Pre-assembled for installation of modules and CombiLine Modules;DISTRIBUTIONBOARD;IfcElectricDistributionPoint;1025;1375;202.5;1400;617.5;1;1;512.5;9;;;;550;0;12.11;EC000058;4;1;215;A49B - 432 modules 1400x1050x215 media WiFi;ABB;499.1;1025;Ventilated metal door WiFi;120;A49B Wall Cab.4PW9R basic media WiFi;215;IP44;0;0;© Stabiplan International BV;www.MEPcontent.com;400;In combination with earthing set (accessory) we can achieve protection class 1;EL_PANEL;;249.82;500;12.11;1027;60;A49B - 432 modules 1400x1050x215 media WiFi;A49B Wall Cab.4PW9R basic media WiFi;;Internal use;EL_MODELPARTSYSTEM_MC;E_Distribution Panel_MEPcontent_ABB_Right Door_INT-EN_Shared : CTW29S;E_Distribution Panel_MEPcontent_ABB_Left Door_INT-EN_Shared : CTB29;E_Distribution Panel_MEPcontent_ABB_Trim Frame CR19-59_INT-EN_Shared : CR49
A49B - 432 modules 1400x1050x215 empty with door;1026.8;1050;;;Color RAL 9016;www.stabiplan.com;12.5;1;111.3;111.3;111.3;111.3;www.stabiplan.com;0;300;UNKNOWN;;432;0;0;0;0;0;0;1;550;2017;400;125;9016;Double insulated;ABB;3;4;;Sheet steel;https://new.abb.com/products/2CPX052091R9999;2CPX052091R9999;DISTRIBUTION_PANEL;;1;550;;Pre-assembled for installation of modules and CombiLine Modules;DISTRIBUTIONBOARD;IfcElectricDistributionPoint;1025;1375;202.5;1400;617.5;1;1;512.5;9;;;;550;0;12.11;EC000058;4;1;215;A49B - 432 modules 1400x1050x215 empty with door;ABB;499.1;1025;Metal door;120;A49B Wall Cab.4PW9R basic empty with door;215;IP44;0;0;© Stabiplan International BV;www.MEPcontent.com;400;In combination with earthing set (accessory) we can achieve protection class 1;EL_PANEL;;249.82;500;12.11;1027;60;A49B - 432 modules 1400x1050x215 empty with door;A49B Wall Cab.4PW9R basic empty with door;;Internal use;EL_MODELPARTSYSTEM_MC;E_Distribution Panel_MEPcontent_ABB_Right Door_INT-EN_Shared : CTB29S;E_Distribution Panel_MEPcontent_ABB_Left Door_INT-EN_Shared : CTB29;E_Distribution Panel_MEPcontent_ABB_Trim Frame CR19-59_INT-EN_Shared : CR49
A59B - 540 modules 1400x1300x215 empty without door;1276.8;1300;;;Color RAL 9016;www.stabiplan.com;12.5;1;111.3;111.3;111.3;111.3;www.stabiplan.com;0;300;UNKNOWN;;540;0;0;0;0;0;0;1;800;2017;400;125;9016;Double insulated;ABB;3;5;;Sheet steel;https://new.abb.com/products/2CPX052092R9999;2CPX052092R9999;DISTRIBUTION_PANEL;;1;550;;Pre-assembled for installation of modules and CombiLine Modules;DISTRIBUTIONBOARD;IfcElectricDistributionPoint;1275;1375;202.5;1400;617.5;1;0;637.5;9;;;;800;0;12.11;EC000058;4;0;215;A59B - 540 modules 1400x1300x215 empty without door;ABB;499.1;1275;Without door;;A59B Wall Cab.5PW9R basic empty without door;215;IP30;0;0;© Stabiplan International BV;www.MEPcontent.com;400;In combination with earthing set (accessory) we can achieve protection class 1;EL_PANEL;;249.82;500;12.11;1277;60;A59B - 540 modules 1400x1300x215 empty without door;A59B Wall Cab.5PW9R basic empty without door;;Internal use;EL_MODELPARTSYSTEM_MC;E_Distribution Panel_MEPcontent_ABB_Right Door_INT-EN_Shared : CTB29S;E_Distribution Panel_MEPcontent_ABB_Left Door_INT-EN_Shared : CTB29;E_Distribution Panel_MEPcontent_ABB_Trim Frame CR19-59_INT-EN_Shared : CR59
A59B - 540 modules 1400x1300x215 transparent door;1276.8;1300;;;Color RAL 9016;www.stabiplan.com;12.5;1;111.3;111.3;111.3;111.3;www.stabiplan.com;0;300;UNKNOWN;;540;0;0;0;0;0;0;1;800;2017;400;125;9016;Double insulated;ABB;3;5;;Sheet steel;https://new.abb.com/products/2CPX052092R9999;2CPX052092R9999;DISTRIBUTION_PANEL;;1;550;;Pre-assembled for installation of modules and CombiLine Modules;DISTRIBUTIONBOARD;IfcElectricDistributionPoint;1275;1375;202.5;1400;617.5;1;1;637.5;9;;;;800;0;12.11;EC000058;4;1;215;A59B - 540 modules 1400x1300x215 transparent door;ABB;499.1;1275;Transparent door;120;A59B Wall Cab.5PW9R basic transparent door;215;IP44;0;0;© Stabiplan International BV;www.MEPcontent.com;400;In combination with earthing set (accessory) we can achieve protection class 1;EL_PANEL;;249.82;500;12.11;1277;60;A59B - 540 modules 1400x1300x215 transparent door;A59B Wall Cab.5PW9R basic transparent door;;Internal use;EL_MODELPARTSYSTEM_MC;E_Distribution Panel_MEPcontent_ABB_Right Door_INT-EN_Shared : CTT29S;E_Distribution Panel_MEPcontent_ABB_Left Door_INT-EN_Shared : CTT29;E_Distribution Panel_MEPcontent_ABB_Trim Frame CR19-59_INT-EN_Shared : CR59
A59B - 540 modules 1400x1300x215 media ventilated;1276.8;1300;;;Color RAL 9016;www.stabiplan.com;12.5;1;111.3;111.3;111.3;111.3;www.stabiplan.com;0;300;UNKNOWN;;540;0;0;0;0;0;0;1;800;2017;400;125;9016;Double insulated;ABB;3;5;;Sheet steel;https://new.abb.com/products/2CPX052092R9999;2CPX052092R9999;DISTRIBUTION_PANEL;;1;550;;Pre-assembled for installation of modules and CombiLine Modules;DISTRIBUTIONBOARD;IfcElectricDistributionPoint;1275;1375;202.5;1400;617.5;1;1;637.5;9;;;;800;0;12.11;EC000058;4;1;215;A59B - 540 modules 1400x1300x215 media ventilated;ABB;499.1;1275;Ventilated metal door;120;A59B Wall Cab.5PW9R basic media ventilated;215;IP44;0;0;© Stabiplan International BV;www.MEPcontent.com;400;In combination with earthing set (accessory) we can achieve protection class 1;EL_PANEL;;249.82;500;12.11;1277;60;A59B - 540 modules 1400x1300x215 media ventilated;A59B Wall Cab.5PW9R basic media ventilated;;Internal use;EL_MODELPARTSYSTEM_MC;E_Distribution Panel_MEPcontent_ABB_Right Door_INT-EN_Shared : CTL29S;E_Distribution Panel_MEPcontent_ABB_Left Door_INT-EN_Shared : CTB29;E_Distribution Panel_MEPcontent_ABB_Trim Frame CR19-59_INT-EN_Shared : CR59
A59B - 540 modules 1400x1300x215 media WiFi;1276.8;1300;;;Color RAL 9016;www.stabiplan.com;12.5;1;111.3;111.3;111.3;111.3;www.stabiplan.com;0;300;UNKNOWN;;540;0;0;0;0;0;0;1;800;2017;400;125;9016;Double insulated;ABB;3;5;;Sheet steel;https://new.abb.com/products/2CPX052092R9999;2CPX052092R9999;DISTRIBUTION_PANEL;;1;550;;Pre-assembled for installation of modules and CombiLine Modules;DISTRIBUTIONBOARD;IfcElectricDistributionPoint;1275;1375;202.5;1400;617.5;1;1;637.5;9;;;;800;0;12.11;EC000058;4;1;215;A59B - 540 modules 1400x1300x215 media WiFi;ABB;499.1;1275;Ventilated metal door WiFi;120;A59B Wall Cab.5PW9R basic media WiFi;215;IP44;0;0;© Stabiplan International BV;www.MEPcontent.com;400;In combination with earthing set (accessory) we can achieve protection class 1;EL_PANEL;;249.82;500;12.11;1277;60;A59B - 540 modules 1400x1300x215 media WiFi;A59B Wall Cab.5PW9R basic media WiFi;;Internal use;EL_MODELPARTSYSTEM_MC;E_Distribution Panel_MEPcontent_ABB_Right Door_INT-EN_Shared : CTW29S;E_Distribution Panel_MEPcontent_ABB_Left Door_INT-EN_Shared : CTB29;E_Distribution Panel_MEPcontent_ABB_Trim Frame CR19-59_INT-EN_Shared : CR59
A59B - 540 modules 1400x1300x215 empty with door;1276.8;1300;;;Color RAL 9016;www.stabiplan.com;12.5;1;111.3;111.3;111.3;111.3;www.stabiplan.com;0;300;UNKNOWN;;540;0;0;0;0;0;0;1;800;2017;400;125;9016;Double insulated;ABB;3;5;;Sheet steel;https://new.abb.com/products/2CPX052092R9999;2CPX052092R9999;DISTRIBUTION_PANEL;;1;550;;Pre-assembled for installation of modules and CombiLine Modules;DISTRIBUTIONBOARD;IfcElectricDistributionPoint;1275;1375;202.5;1400;617.5;1;1;637.5;9;;;;800;0;12.11;EC000058;4;1;215;A59B - 540 modules 1400x1300x215 empty with door;ABB;499.1;1275;Metal door;120;A59B Wall Cab.5PW9R basic empty with door;215;IP44;0;0;© Stabiplan International BV;www.MEPcontent.com;400;In combination with earthing set (accessory) we can achieve protection class 1;EL_PANEL;;249.82;500;12.11;1277;60;A59B - 540 modules 1400x1300x215 empty with door;A59B Wall Cab.5PW9R basic empty with door;;Internal use;EL_MODELPARTSYSTEM_MC;E_Distribution Panel_MEPcontent_ABB_Right Door_INT-EN_Shared : CTB29S;E_Distribution Panel_MEPcontent_ABB_Left Door_INT-EN_Shared : CTB29;E_Distribution Panel_MEPcontent_ABB_Trim Frame CR19-59_INT-EN_Shared : CR59
