;Width Safe##LENGTH##MILLIMETERS;Width (mm)##LENGTH##MILLIMETERS;Wholesaler Art. No.##OTHER##;Wholesaler##OTHER##;White##OTHER##;Watermarked By##OTHER##;Wall Thickness##LENGTH##MILLIMETERS;Upper Width 4##LENGTH##MILLIMETERS;Upper Width 3##LENGTH##MILLIMETERS;Upper Width 2##LENGTH##MILLIMETERS;Upper Width 1##LENGTH##MILLIMETERS;URL##OTHER##;Top Clearance##LENGTH##MILLIMETERS;Stabu Code##OTHER##;Space Units [SU]##OTHER##;Phase##OTHER##;Show Service Area##OTHER##;Right Clearance##LENGTH##MILLIMETERS;Revit Version##OTHER##;Rated Current In [A]##OTHER##;RAL-Number##OTHER##;Protection Class##OTHER##;Product Line##OTHER##;Phase##OTHER##;Panel Width (PW)##OTHER##;Grid Units (GU)##OTHER##;Material of Enclosures##OTHER##;Manufacturer URL##OTHER##;Manufacturer Art. No.##OTHER##;MEPcontent Class##OTHER##;Left Clearance##LENGTH##MILLIMETERS;Internal Art. No.##OTHER##;IFCExportType##OTHER##;IFCExportAs##OTHER##;Height (mm)##LENGTH##MILLIMETERS;Handle Height##LENGTH##MILLIMETERS;Handle##OTHER##;Half Width##LENGTH##MILLIMETERS;GTIN##OTHER##;GLN##OTHER##;Function Code##OTHER##;Front Clearance##LENGTH##MILLIMETERS;Family Version##OTHER##;Interior Fitting##OTHER##;ETIM Article Class##OTHER##;EMCS Version##OTHER##;Double Door##OTHER##;Model##OTHER##;Manufacturer##OTHER##;Door Type##OTHER##;Door Opening Angle [degrees]##OTHER##;Description##OTHER##;Depth (mm)##LENGTH##MILLIMETERS;Degree of Protection##OTHER##;Custom##OTHER##;Copyright##OTHER##;Content Supplier URL##OTHER##;Connection Voltage##ELECTRICAL_POTENTIAL##VOLTS;CB-NL Class##OTHER##;Bottom Width##LENGTH##MILLIMETERS;Bottom Clearance##LENGTH##MILLIMETERS;Base Family Version##OTHER##;Back Clearance##LENGTH##MILLIMETERS;Article Type##OTHER##;Article Description##OTHER##;Area of Application##OTHER##;Class of Protection with Accessories##OTHER##;Rated Operational Voltage Ue [V] AC##OTHER##;Locking Type — Lock##OTHER##
A16 - IP44 72 modules 950x300x215;276.8;300;;;Color RAL 9016;www.stabiplan.com;12.5;111.3;111.3;111.3;111.3;www.stabiplan.com;300;;72;3;0;800;2017;250;9016;Double insulated;ABB;3;1;6;Sheet steel;https://new.abb.com/products/2CPX052025R9999;2CPX052025R9999;DISTRIBUTION_PANEL;250;;IfcElectricDistributionPoint;DISTRIBUTIONBOARD;950;392.5;1;137.5;;;E6211;300;12.11;Pre-assembled for installation of metering-, modules, Combi-Sets, CombiLine-Module on EDF-mounting frame;EC000058;4;0;A16 - IP44 72 modules 950x300x215;ABB;Metal door;120;A16 Wall Cabinet 1PW6R PC2 IP44;215;IP44;0;© Stabiplan International BV;www.MEPcontent.com;400;;249.8;500;12.11;60;A16 - IP44 72 modules 950x300x215;A16 Wall Cabinet 1PW6R PC2 IP44;Internal use;;;
A26 - IP44 144 modules 950x550x215;526.8;550;;;Color RAL 9016;www.stabiplan.com;12.5;111.3;111.3;111.3;361.3;www.stabiplan.com;300;;144;3;0;800;2017;250;9016;Double insulated;ABB;3;2;6;Sheet steel;https://new.abb.com/products/2CPX052026R9999;2CPX052026R9999;DISTRIBUTION_PANEL;250;;IfcElectricDistributionPoint;DISTRIBUTIONBOARD;950;392.5;1;137.5;;;E6211;550;12.11;Pre-assembled for installation of metering-, modules, Combi-Sets, CombiLine-Module on EDF-mounting frame;EC000058;4;0;A26 - IP44 144 modules 950x550x215;ABB;Metal door;120;A26 Wall Cabinet 2PW6R PC2 IP44;215;IP44;0;© Stabiplan International BV;www.MEPcontent.com;400;;249.8;500;12.11;60;A26 - IP44 144 modules 950x550x215;A26 Wall Cabinet 2PW6R PC2 IP44;Internal use;;;
A36 - IP44 216 modules 950x800x215;776.8;800;;;Color RAL 9016;www.stabiplan.com;12.5;111.3;111.3;611.3;361.3;www.stabiplan.com;300;;216;3;0;800;2017;250;9016;Double insulated;ABB;3;3;6;Sheet steel;https://new.abb.com/products/2CPX052027R9999;2CPX052027R9999;DISTRIBUTION_PANEL;300;;IfcElectricDistributionPoint;DISTRIBUTIONBOARD;950;392.5;1;137.5;;;E6211;550;12.11;Pre-assembled for installation of metering-, modules, Combi-Sets, CombiLine-Module on EDF-mounting frame;EC000058;4;1;A36 - IP44 216 modules 950x800x215;ABB;Metal door;120;A36 Wall Cabinet 3PW6R PC2 IP44;215;IP44;0;© Stabiplan International BV;www.MEPcontent.com;400;;249.8;500;12.11;60;A36 - IP44 216 modules 950x800x215;A36 Wall Cabinet 3PW6R PC2 IP44;Internal use;;;
A46 - IP44 288 modules 950x1050x215;1026.8;1050;;;Color RAL 9016;www.stabiplan.com;12.5;111.3;861.3;611.3;361.3;www.stabiplan.com;300;;288;3;0;800;2017;250;9016;Double insulated;ABB;3;4;6;Sheet steel;https://new.abb.com/products/2CPX052028R9999;2CPX052028R9999;DISTRIBUTION_PANEL;550;;IfcElectricDistributionPoint;DISTRIBUTIONBOARD;950;392.5;1;137.5;;;E6211;550;12.11;Pre-assembled for installation of metering-, modules, Combi-Sets, CombiLine-Module on EDF-mounting frame;EC000058;4;1;A46 - IP44 288 modules 950x1050x215;ABB;Metal door;120;A46 Wall Cabinet 4PW6R PC2 IP44;215;IP44;0;© Stabiplan International BV;www.MEPcontent.com;400;;249.8;500;12.11;60;A46 - IP44 288 modules 950x1050x215;A46 Wall Cabinet 4PW6R PC2 IP44;Internal use;;;
A56 - IP44 360 modules 950x1300x215;1276.8;1300;;;Color RAL 9016;www.stabiplan.com;12.5;1111.3;861.3;611.3;361.3;www.stabiplan.com;300;;360;3;0;800;2017;250;9016;Double insulated;ABB;3;5;6;Sheet steel;https://new.abb.com/products/2CPX052029R9999;2CPX052029R9999;DISTRIBUTION_PANEL;550;;IfcElectricDistributionPoint;DISTRIBUTIONBOARD;950;392.5;1;137.5;;;E6211;800;12.11;Pre-assembled for installation of metering-, modules, Combi-Sets, CombiLine-Module on EDF-mounting frame;EC000058;4;1;A56 - IP44 360 modules 950x1300x215;ABB;Metal door;120;A56 Wall Cabinet 5PW6R PC2 IP44;215;IP44;0;© Stabiplan International BV;www.MEPcontent.com;400;;249.8;500;12.11;60;A56 - IP44 360 modules 950x1300x215;A56 Wall Cabinet 5PW6R PC2 IP44;Internal use;;;
A16D - IP54 72 modules 950x300x215;276.8;300;;;Color RAL 9016;www.stabiplan.com;12.5;111.3;111.3;111.3;111.3;www.stabiplan.com;300;;72;3;0;800;2017;250;9016;Double insulated;ABB;3;1;6;Sheet steel;https://new.abb.com/products/2CPX052095R9999;2CPX052095R9999;DISTRIBUTION_PANEL;250;;IfcElectricDistributionPoint;DISTRIBUTIONBOARD;950;392.5;1;137.5;;;E6211;300;12.11;Pre-assembled for installation of metering-, modules, Combi-Sets, CombiLine-Module on EDF-mounting frame;EC000058;4;0;A16D - IP54 72 modules 950x300x215;ABB;Metal door;120;A16D Wall Cabinet 1PW6R PC2 IP54;215;IP54;0;© Stabiplan International BV;www.MEPcontent.com;400;;249.8;500;12.11;60;A16D - IP54 72 modules 950x300x215;A16D Wall Cabinet 1PW6R PC2 IP54;Internal use;;;
A26D - IP54 144 modules 950x550x215;526.8;550;;;Color RAL 9016;www.stabiplan.com;12.5;111.3;111.3;111.3;361.3;www.stabiplan.com;300;;144;3;0;800;2017;250;9016;Double insulated;ABB;3;2;6;Sheet steel;https://new.abb.com/products/2CPX052096R9999;2CPX052096R9999;DISTRIBUTION_PANEL;250;;IfcElectricDistributionPoint;DISTRIBUTIONBOARD;950;392.5;1;137.5;;;E6211;550;12.11;Pre-assembled for installation of metering-, modules, Combi-Sets, CombiLine-Module on EDF-mounting frame;EC000058;4;0;A26D - IP54 144 modules 950x550x215;ABB;Metal door;120;A26D Wall Cabinet 2PW6R PC2 IP54;215;IP54;0;© Stabiplan International BV;www.MEPcontent.com;400;;249.8;500;12.11;60;A26D - IP54 144 modules 950x550x215;A26D Wall Cabinet 2PW6R PC2 IP54;Internal use;;;
A36D - IP54 216 modules 950x800x215;776.8;800;;;Color RAL 9016;www.stabiplan.com;12.5;111.3;111.3;611.3;361.3;www.stabiplan.com;300;;216;3;0;800;2017;250;9016;Double insulated;ABB;3;3;6;Sheet steel;https://new.abb.com/products/2CPX052097R9999;2CPX052097R9999;DISTRIBUTION_PANEL;300;;IfcElectricDistributionPoint;DISTRIBUTIONBOARD;950;392.5;1;137.5;;;E6211;550;12.11;Pre-assembled for installation of metering-, modules, Combi-Sets, CombiLine-Module on EDF-mounting frame;EC000058;4;1;A36D - IP54 216 modules 950x800x215;ABB;Metal door;120;A36D Wall Cabinet 3PW6R PC2 IP54;215;IP54;0;© Stabiplan International BV;www.MEPcontent.com;400;;249.8;500;12.11;60;A36D - IP54 216 modules 950x800x215;A36D Wall Cabinet 3PW6R PC2 IP54;Internal use;;;
A46D - IP54 288 modules 950x1050x215;1026.8;1050;;;Color RAL 9016;www.stabiplan.com;12.5;111.3;861.3;611.3;361.3;www.stabiplan.com;300;;288;3;0;800;2017;250;9016;Double insulated;ABB;3;4;6;Sheet steel;https://new.abb.com/products/2CPX052098R9999;2CPX052098R9999;DISTRIBUTION_PANEL;550;;IfcElectricDistributionPoint;DISTRIBUTIONBOARD;950;392.5;1;137.5;;;E6211;550;12.11;Pre-assembled for installation of metering-, modules, Combi-Sets, CombiLine-Module on EDF-mounting frame;EC000058;4;1;A46D - IP54 288 modules 950x1050x215;ABB;Metal door;120;A46D Wall Cabinet 4PW6R PC2 IP54;215;IP54;0;© Stabiplan International BV;www.MEPcontent.com;400;;249.8;500;12.11;60;A46D - IP54 288 modules 950x1050x215;A46D Wall Cabinet 4PW6R PC2 IP54;Internal use;;;
A56D - IP54 360 modules 950x1300x215;1276.8;1300;;;Color RAL 9016;www.stabiplan.com;12.5;1111.3;861.3;611.3;361.3;www.stabiplan.com;300;;360;3;0;800;2017;250;9016;Double insulated;ABB;3;5;6;Sheet steel;https://new.abb.com/products/2CPX052099R9999;2CPX052099R9999;DISTRIBUTION_PANEL;550;;IfcElectricDistributionPoint;DISTRIBUTIONBOARD;950;392.5;1;137.5;;;E6211;800;12.11;Pre-assembled for installation of metering-, modules, Combi-Sets, CombiLine-Module on EDF-mounting frame;EC000058;4;1;A56D - IP54 360 modules 950x1300x215;ABB;Metal door;120;A56D Wall Cabinet 5PW6R PC2 IP54;215;IP54;0;© Stabiplan International BV;www.MEPcontent.com;400;;249.8;500;12.11;60;A56D - IP54 360 modules 950x1300x215;A56D Wall Cabinet 5PW6R PC2 IP54;Internal use;;;
